### RF_PLL_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
26 | RW | PLL_CTRL_DISABLE_CHP_SBS | Charge-pump disabling during sub-band selection (FLL and frequency ratios)
25 | RW | PLL_CTRL_PLL_RX_48MEG | PLL frequency
24 | RW | PLL_CTRL_SWCAP_TX_SAME_RX | Registers for Rx and Tx modes swcap in case of swcap_fsm=1
23 | RW | PLL_CTRL_SWCAP_FSM | Selection of the swcap_fsm register
22 | RW | PLL_CTRL_DLL_RSTB | Reset signal of the DLL (active low)
21:18 | RW | PLL_CTRL_VCO_SUBBAND_TRIM | VCO sub-band selection bits
17 | RW | PLL_CTRL_SUB_SEL_OFFS_EN | Add offset to sub-band selection comparator
16 | RW | PLL_CTRL_DIV2_CLKVCO_TEST_EN | VCO signal divided by the programmable divider
15 | RW | PLL_CTRL_VCODIV_CLK_TEST_EN | Output on GPIO the VCO signal divided by the programmable divider
13 | RW | PLL_CTRL_CHP_DEAD_ZONE_EN | Charge-pump dead zone
12:11 | RW | PLL_CTRL_CHP_CURR_OFF_TRIM_TX | Charge-pump offset current values selection bits in Tx mode
10:9 | RW | PLL_CTRL_CHP_CURR_OFF_TRIM_RX | Charge-pump offset current values selection bits in Rx mode
8 | RW | PLL_CTRL_HIGH_BW_FILTER_EN_TX | PLL filter high bandwidth needed in Tx mode
7 | RW | PLL_CTRL_HIGH_BW_FILTER_EN_RX | PLL filter high bandwidth needed in Rx mode
6 | RW | PLL_CTRL_FAST_CHP_EN_TX | High current output of the charge-pump for PLL Tx high bandwidth mode
5 | RW | PLL_CTRL_FAST_CHP_EN_RX | High current output of the charge-pump for PLL Rx high bandwidth mode
4:3 | RW | PLL_CTRL_CHP_MODE_TRIM | Select the frequency inside sub-band selection
2 | RW | PLL_CTRL_CHP_CMC_EN | Common mode control block of the charge-pump
1 | RW | PLL_CTRL_CHP_CURR_OFF_EN_TX | Charge-pump offset current in Tx mode
0 | RW | PLL_CTRL_CHP_CURR_OFF_EN_RX | Charge-pump offset current in Rx mode

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
26 | PLL_CTRL_DISABLE_CHP_SBS | PLL_CTRL_2_DISABLE_CHP_SBS_DISABLE | Charge-pump is enabled during the sub-band selection | 0x0*
|  | PLL_CTRL_2_DISABLE_CHP_SBS_ENABLE | Charge-pump is disabled during the sub-band selection | 0x1
25 | PLL_CTRL_PLL_RX_48MEG | PLL_CTRL_2_PLL_RX_48MEG_24 | PLL is set to 24MHz in Rx | 0x0
|  | PLL_CTRL_2_PLL_RX_48MEG_48 | PLL is set to 48MHz in Rx | 0x1*
24 | PLL_CTRL_SWCAP_TX_SAME_RX | PLL_CTRL_2_SWCAP_TX_SAME_RX_DISABLE | The register for Rx and Tx swcap is not the same | 0x0*
|  | PLL_CTRL_2_SWCAP_TX_SAME_RX_ENABLE | The register for Rx and Tx swcap is the same | 0x1
23 | PLL_CTRL_SWCAP_FSM | PLL_CTRL_2_SWCAP_FSM_DISABLE | Don't use the swcap_fsm register as reference for the sub-band selection | 0x0
|  | PLL_CTRL_2_SWCAP_FSM_ENABLE | Use the swcap_fsm register as reference for the sub-band selection | 0x1*
22 | PLL_CTRL_DLL_RSTB | PLL_CTRL_2_DLL_RSTB_RESET | Reset the DLL | 0x0
|  | PLL_CTRL_2_DLL_RSTB_NO_RESET | Don't reset the DLL | 0x1*
21:18 | PLL_CTRL_VCO_SUBBAND_TRIM | PLL_CTRL_VCO_SUBBAND_TRIM_DEFAULT |  | 0x0*
17 | PLL_CTRL_SUB_SEL_OFFS_EN | PLL_CTRL_1_SUB_SEL_OFFS_EN_DISABLE | Don't add offset to sub-band selection comparator | 0x0*
|  | PLL_CTRL_1_SUB_SEL_OFFS_EN_ENABLE | Add offset to sub-band selection comparator | 0x1
16 | PLL_CTRL_DIV2_CLKVCO_TEST_EN | PLL_CTRL_1_DIV2_CLKVCO_TEST_EN_1 | Division ratio set to 1 | 0x0*
|  | PLL_CTRL_1_DIV2_CLKVCO_TEST_EN_2 | Division ratio set to 2 (before to be outputted to ck_div_test) | 0x1
15 | PLL_CTRL_VCODIV_CLK_TEST_EN | PLL_CTRL_1_VCODIV_CLK_TEST_EN_DISABLE | Disable to output on GPIO the VCO signal divided by the programmable divider | 0x0*
|  | PLL_CTRL_ENABLE_VCODIV_CLK_TEST_EN_ENABLE | Enable to output on GPIO the VCO signal divided by the programmable divider | 0x1
13 | PLL_CTRL_CHP_DEAD_ZONE_EN | PLL_CTRL_1_CHP_DEAD_ZONE_EN_DISABLE | Disable charge-pump dead zone | 0x0*
|  | PLL_CTRL_ENABLE_CHP_DEAD_ZONE_EN_ENABLE | Enable charge-pump dead zone | 0x1
12:11 | PLL_CTRL_CHP_CURR_OFF_TRIM_TX | PLL_CTRL_1_CHP_CURR_OFF_TRIM_TX_15 | d_phi=15 | 0x0
|  | PLL_CTRL_1_CHP_CURR_OFF_TRIM_TX_22 | d_phi=22.5 | 0x1
|  | PLL_CTRL_1_CHP_CURR_OFF_TRIM_TX_30 | d_phi = 30 | 0x2
|  | PLL_CTRL_1_CHP_CURR_OFF_TRIM_TX_60 | d_phi = 60 | 0x3*
10:9 | PLL_CTRL_CHP_CURR_OFF_TRIM_RX | PLL_CTRL_1_CHP_CURR_OFF_TRIM_RX_15 | d_phi=15 | 0x0
|  | PLL_CTRL_1_CHP_CURR_OFF_TRIM_RX_22 | d_phi=22.5 | 0x1
|  | PLL_CTRL_1_CHP_CURR_OFF_TRIM_RX_30 | d_phi = 30 | 0x2
|  | PLL_CTRL_1_CHP_CURR_OFF_TRIM_RX_60 | d_phi = 60 | 0x3*
8 | PLL_CTRL_HIGH_BW_FILTER_EN_TX | PLL_CTRL_HIGH_BW_FILTER_EN_TX_DISABLE | Disable the PLL filter high bandwidth needed in TX | 0x0
|  | PLL_CTRL_HIGH_BW_FILTER_EN_TX_ENABLE | Enable the PLL filter high bandwidth needed in TX | 0x1*
7 | PLL_CTRL_HIGH_BW_FILTER_EN_RX | PLL_CTRL_HIGH_BW_FILTER_EN_RX_DISABLE | Disable the PLL filter high bandwidth needed in RX | 0x0*
|  | PLL_CTRL_HIGH_BW_FILTER_EN_RX_ENABLE | Enable the PLL filter high bandwidth needed in RX | 0x1
6 | PLL_CTRL_FAST_CHP_EN_TX | PLL_CTRL_FAST_CHP_EN_TX_DISABLE | Disable the high current output of the charge-pump in TX | 0x0
|  | PLL_CTRL_FAST_CHP_EN_TX_ENABLE | Enable the high current output of the charge-pum in TX | 0x1*
5 | PLL_CTRL_FAST_CHP_EN_RX | PLL_CTRL_FAST_CHP_EN_RX_DISABLE | Disable the high current output of the charge-pump in RX | 0x0*
|  | PLL_CTRL_FAST_CHP_EN_RX_ENABLE | Enable the high current output of the charge-pump in RX | 0x1
4:3 | PLL_CTRL_CHP_MODE_TRIM | PLL_CTRL_CHP_MODE_TRIM_MIN_FREQ | Minimum frequency inside sub-band selection | 0x0*
|  | PLL_CTRL_CHP_MODE_TRIM_MED_FREQ | Medium frequency inside sub-band selection | 0x1
|  | PLL_CTRL_CHP_MODE_TRIM_MAX_FREQ | Maximum frequency inside sub-band selection | 0x2
2 | PLL_CTRL_CHP_CMC_EN | PLL_CTRL_CHP_CMC_EN_DISABLE | Disable the common mode control block of the charge-pump | 0x0
|  | PLL_CTRL_CHP_CMC_EN_ENABLE | Enable the common mode control block of the charge-pump | 0x1*
1 | PLL_CTRL_CHP_CURR_OFF_EN_TX | PLL_CTRL_CHP_CURR_OFF_EN_TX_DISABLE | Disable the charge-pump offset current in TX | 0x0
|  | PLL_CTRL_CHP_CURR_OFF_EN_TX_ENABLE | Enable the charge-pump offset current in TX | 0x1*
0 | PLL_CTRL_CHP_CURR_OFF_EN_RX | PLL_CTRL_CHP_CURR_OFF_EN_RX_DISABLE | Disable the charge-pump offset current in RX | 0x0*
|  | PLL_CTRL_CHP_CURR_OFF_EN_RX_ENABLE | Enable the charge-pump offset current in RX | 0x1