### SENSOR_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | W | RESET | Reset the Sensor interface (SAR and Pulse Counter)
12 | R | STATE | Sensor state
8 | R | STATUS | Sensor status
0 | RW | ENABLE | Sensor

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | RESET | SENSOR_RESET | The sensor timer counter, the SAR-ADC analog, the sensor enable and the pulse counter are reset. | 0x1
12 | STATE | DELAY_STATUS | Sensor in delay state or in idle state | 0x0*
|  | COUNT_STATUS | Sensor in count state | 0x1
8 | STATUS | SENSOR_IDLE | Sensor state machine in idle mode | 0x0*
|  | SENSOR_RUNNING | Sensor state machine in active mode | 0x1
0 | ENABLE | SENSOR_DISABLE | Sensor disables | 0x0*
|  | SENSOR_ENABLE | Sensor enables | 0x1