### BB_RADIOTXRXTIM0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
22:16 | RW | RFRXTMDA0 | RF Rx test mode delay adjustment for uncoded PHY at 1Mbps
14:8 | RW | RXPATHDLY0 | Rx path delay (in us) for uncoded PHY at 1Mbps
6:0 | RW | TXPATHDLY0 | Rx path delay (in us) for uncoded PHY at 1Mbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
22:16 | RFRXTMDA0 | RFRXTMDA0_0 |  | 0x0*
14:8 | RXPATHDLY0 | RXPATHDLY0_0 |  | 0x0*
6:0 | TXPATHDLY0 | TXPATHDLY0_0 |  | 0x0*