### NVIC_IABR1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
24 | R | DMA3 | Set the DMA3 interrupt as active
23 | R | DMA2 | Set the DMA2 interrupt as active
22 | R | DMA1 | Set the DMA1 interrupt as active
21 | R | DMA0 | Set the DMA0 interrupt as active
20 | R | ACCESS_ERROR | Set the ACCESS_ERROR interrupt as active
19 | R | FLASH0_ECC | Set the FLASH0_ECC interrupt as active
18 | R | FLASH0_COPY | Set the FLASH0_COPY interrupt as active
17 | R | RF_RXFIFO | Set the RF_RXFIFO interrupt as active
16 | R | RF_TXFIFO | Set the RF_TXFIFO interrupt as active
15 | R | RF_SYNC | Set the RF_SYNC interrupt as active
14 | R | RF_IRQ_RECEIVED | Set the RF_IRQ_RECEIVED interrupt as active
13 | R | RF_RXSTOP | Set the RF_RXSTOP interrupt as active
12 | R | RF_TX | Set the RF_TX interrupt as active
11 | R | TOF | Set the TOF interrupt as active
10 | R | BLE_COEX_RX_TX | Set the BLE_COEX_RX_TX interrupt as active
9 | R | BLE_COEX_IN_PROCESS | Set the BLE_COEX_IN_PROCESS interrupt as active
8 | R | BLE_ERROR | Set the BLE_ERROR interrupt as active
7 | R | BLE_FIFO | Set the BLE_FIFO interrupt as active
6 | R | BLE_HSLOT | Set the BLE_HSLOT interrupt as active
5 | R | BLE_SLP | Set the BLE_SLP interrupt as active
4 | R | BLE_CRYPT | Set the BLE_CRYPT interrupt as active
3 | R | BLE_TIMESTAMP_TGT2 | Set the BLE_TIMESTAMP_TGT2 interrupt as active
2 | R | BLE_TIMESTAMP_TGT1 | Set the BLE_TIMESTAMP_TGT1 interrupt as active
1 | R | BLE_FINETGT | Set the BLE_FINETGT interrupt as active
0 | R | BLE_SW | Set the BLE_SW interrupt as active

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
24 | DMA3 | NVIC_DMA3_INT_ACTIVE | The NVIC_DMA3_INT_ACTIVE interrupt is active | 0x1
23 | DMA2 | NVIC_DMA2_INT_ACTIVE | The NVIC_DMA2_INT_ACTIVE interrupt is active | 0x1
22 | DMA1 | NVIC_DMA1_INT_ACTIVE | The NVIC_DMA1_INT_ACTIVE interrupt is active | 0x1
21 | DMA0 | NVIC_DMA0_INT_ACTIVE | The NVIC_DMA0_INT_ACTIVE interrupt is active | 0x1
20 | ACCESS_ERROR | NVIC_ACCESS_ERROR_INT_ACTIVE | The NVIC_ACCESS_ERROR_INT_ACTIVE interrupt is active | 0x1
19 | FLASH0_ECC | NVIC_FLASH0_ECC_INT_ACTIVE | The NVIC_FLASH0_ECC_INT_ACTIVE interrupt is active | 0x1
18 | FLASH0_COPY | NVIC_FLASH0_COPY_INT_ACTIVE | The NVIC_FLASH0_COPY_INT_ACTIVE interrupt is active | 0x1
17 | RF_RXFIFO | NVIC_RF_RXFIFO_INT_ACTIVE | The NVIC_RF_RXFIFO_INT_ACTIVE interrupt is active | 0x1
16 | RF_TXFIFO | NVIC_RF_TXFIFO_INT_ACTIVE | The NVIC_RF_TXFIFO_INT_ACTIVE interrupt is active | 0x1
15 | RF_SYNC | NVIC_RF_SYNC_INT_ACTIVE | The NVIC_RF_SYNC_INT_ACTIVE interrupt is active | 0x1
14 | RF_IRQ_RECEIVED | NVIC_RF_IRQ_RECEIVED_INT_ACTIVE | The NVIC_RF_IRQ_RECEIVED_INT_ACTIVE interrupt is active | 0x1
13 | RF_RXSTOP | NVIC_RF_RXSTOP_INT_ACTIVE | The NVIC_RF_RXSTOP_INT_ACTIVE interrupt is active | 0x1
12 | RF_TX | NVIC_RF_TX_INT_ACTIVE | The NVIC_RF_TX_INT_ACTIVE interrupt is active | 0x1
11 | TOF | NVIC_TOF_INT_ACTIVE | The NVIC_TOF_INT_ACTIVE interrupt is active | 0x1
10 | BLE_COEX_RX_TX | NVIC_BLE_COEX_RX_TX_INT_ACTIVE | The NVIC_BLE_COEX_RX_TX_INT_ACTIVE interrupt is active | 0x1
9 | BLE_COEX_IN_PROCESS | NVIC_BLE_COEX_IN_PROCESS_INT_ACTIVE | The NVIC_BLE_COEX_IN_PROCESS_INT_ACTIVE interrupt is active | 0x1
8 | BLE_ERROR | NVIC_BLE_ERROR_INT_ACTIVE | The NVIC_BLE_ERROR_INT_ACTIVE interrupt is active | 0x1
7 | BLE_FIFO | NVIC_BLE_FIFO_INT_ACTIVE | The NVIC_BLE_FIFO_INT_ACTIVE interrupt is active | 0x1
6 | BLE_HSLOT | NVIC_BLE_HSLOT_INT_ACTIVE | The NVIC_BLE_HSLOT_INT_ACTIVE interrupt is active | 0x1
5 | BLE_SLP | NVIC_BLE_SLP_INT_ACTIVE | The NVIC_BLE_SLP_INT_ACTIVE interrupt is active | 0x1
4 | BLE_CRYPT | NVIC_BLE_CRYPT_INT_ACTIVE | The NVIC_BLE_CRYPT_INT_ACTIVE interrupt is active | 0x1
3 | BLE_TIMESTAMP_TGT2 | NVIC_BLE_TIMESTAMP_TGT2_INT_ACTIVE | The NVIC_BLE_TIMESTAMP_TGT2_INT_ACTIVE interrupt is active | 0x1
2 | BLE_TIMESTAMP_TGT1 | NVIC_BLE_TIMESTAMP_TGT1_INT_ACTIVE | The NVIC_BLE_TIMESTAMP_TGT1_INT_ACTIVE interrupt is active | 0x1
1 | BLE_FINETGT | NVIC_BLE_FINETGT_INT_ACTIVE | The NVIC_BLE_FINETGT_INT_ACTIVE interrupt is active | 0x1
0 | BLE_SW | NVIC_BLE_SW_INT_ACTIVE | The NVIC_BLE_SW_INT_ACTIVE interrupt is active | 0x1