### PWM_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
28:24 | W | RESET | PWM[4:0] channel reset
20:16 | R | ENABLE_STATUS | PWM enable status
12:8 | W | DISABLE | Disable the PWM[4:0] channel
4:0 | W | ENABLE | Enable the PWM[4:0] channel

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
28:24 | RESET | PWM0_RESET | Disable the PWM0 channel, reset the PWM_CFG0 and PWM_OFFSET0 registers and the related counter. | 0x1
|  | PWM1_RESET | Disable the PWM1 channel, reset the PWM_CFG1 and PWM_OFFSET1 registers and the related counter. | 0x2
|  | PWM2_RESET | Disable the PWM2 channel, reset the PWM_CFG2 and PWM_OFFSET2 registers and the related counter. | 0x4
|  | PWM3_RESET | Disable the PWM3 channel, reset the PWM_CFG3 and PWM_OFFSET3 registers and the related counter. | 0x8
|  | PWM4_RESET | Disable the PWM4 channel, reset the PWM_CFG4 and PWM_OFFSET4 registers and the related counter. | 0x10
20:16 | ENABLE_STATUS | PWM0_STATUS_DISABLE | PWM0 channel disable | 0x0*
|  | PWM1_STATUS_DISABLE | PWM1 channel disable | 0x0*
|  | PWM2_STATUS_DISABLE | PWM2 channel disable | 0x0*
|  | PWM3_STATUS_DISABLE | PWM3 channel disable | 0x0*
|  | PWM4_STATUS_DISABLE | PWM4 channel disable | 0x0*
|  | PWM0_STATUS_ENABLE | PWM0 channel enable | 0x1
|  | PWM1_STATUS_ENABLE | PWM1 channel enable | 0x2
|  | PWM2_STATUS_ENABLE | PWM2 channel enable | 0x4
|  | PWM3_STATUS_ENABLE | PWM3 channel enable | 0x8
|  | PWM4_STATUS_ENABLE | PWM4 channel enable | 0x10
12:8 | DISABLE | PWM0_DISABLE | Disable the PWM0 channel | 0x1
|  | PWM1_DISABLE | Disable the PWM1 channel | 0x2
|  | PWM2_DISABLE | Disable the PWM2 channel | 0x4
|  | PWM3_DISABLE | Disable the PWM3 channel | 0x8
|  | PWM4_DISABLE | Disable the PWM4 channel | 0x10
4:0 | ENABLE | PWM0_ENABLE | Enable the PWM0 channel | 0x1
|  | PWM1_ENABLE | Enable the PWM1 channel | 0x2
|  | PWM2_ENABLE | Enable the PWM2 channel | 0x4
|  | PWM3_ENABLE | Enable the PWM3 channel | 0x8
|  | PWM4_ENABLE | Enable the PWM4 channel | 0x10