### BB_ADVTIM

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | TX_AUXPTR_THR | Extended advertising AuxPtr threshold value in Tx (granularity 16us)
23:16 | RW | RX_AUXPTR_THR | Extended advertising AuxPtr threshold value in Rx (granularity 16us)
13:0 | RW | ADVINT | Advertising packet interval defining the time interval in between two ADV_xxx packet sent (value in us)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | TX_AUXPTR_THR | TX_AUXPTR_THR_0 |  | 0x0*
23:16 | RX_AUXPTR_THR | RX_AUXPTR_THR_0 |  | 0x0*
13:0 | ADVINT | ADVINT_0 |  | 0x0*