### BB_ENBPRESET

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:21 | RW | TWEXT | Time in low power oscillator cycles allowed for stabilization of the high frequency oscillator following an external wake-up request (signal wakeup_req)
20:10 | RW | TWOSC | Time in low power oscillator cycles allowed for stabilization of the high frequency oscillator when the deep-sleep mode has been left due to sleep-timer expiry (DEEPSLWKUP-DEEPSLTIME])
9:0 | RW | TWRM | Time in low power oscillator cycles allowed for the radio module to leave low-power mode

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:21 | TWEXT | TWEXT_0 |  | 0x0*
20:10 | TWOSC | TWOSC_0 |  | 0x0*
9:0 | TWRM | TWRM_0 |  | 0x0*