### TIMER_CFG1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
12 | RW | CLK_SRC | Clock source
10:8 | RW | MULTI_COUNT | Multi-count value
6:4 | RW | GPIO_INT_SRC | GPIO interrupt source selection
2 | RW | GPIO_INT_MODE | GPIO interrupt capture mode
1 | RW | GPIO_INT_ENABLE | GPIO interrupt capture enable
0 | RW | MODE | Timer mode

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
12 | CLK_SRC | TIMER_SLOWCLK_DIV32 | Timer clock source is SLOWCLK divided by 32 | 0x0*
|  | TIMER_SLOWCLK_DIV2 | Timer clock source is SLOWCLK divided by 2 | 0x1
10:8 | MULTI_COUNT | TIMER_MULTI_COUNT_1 | Stop on 1st Time-out occurrence and issue an interrupt | 0x0*
|  | TIMER_MULTI_COUNT_2 | Stop on 2nd Time-out occurrence and issue an interrupt | 0x1
|  | TIMER_MULTI_COUNT_3 | Stop on 3rd Time-out occurrence and issue an interrupt | 0x2
|  | TIMER_MULTI_COUNT_4 | Stop on 4th Time-out occurrence and issue an interrupt | 0x3
|  | TIMER_MULTI_COUNT_5 | Stop on 5th Time-out occurrence and issue an interrupt | 0x4
|  | TIMER_MULTI_COUNT_6 | Stop on 6th Time-out occurrence and issue an interrupt | 0x5
|  | TIMER_MULTI_COUNT_7 | Stop on 7th Time-out occurrence and issue an interrupt | 0x6
|  | TIMER_MULTI_COUNT_8 | Stop on 8th Time-out occurrence and issue an interrupt | 0x7
6:4 | GPIO_INT_SRC | TIMER_SRC_GPIO_INT0 | Select GPIO interrupt defined in GPIO_INT_CFG0 | 0x0*
|  | TIMER_SRC_GPIO_INT1 | Select GPIO interrupt defined in GPIO_INT_CFG1 | 0x1
|  | TIMER_SRC_GPIO_INT2 | Select GPIO interrupt defined in GPIO_INT_CFG2 | 0x2
|  | TIMER_SRC_GPIO_INT3 | Select GPIO interrupt defined in GPIO_INT_CFG3 | 0x3
2 | GPIO_INT_MODE | TIMER_GPIO_INT_SINGLE | GPIO interrupt single capture mode | 0x0*
|  | TIMER_GPIO_INT_CONTINUOUS | GPIO interrupt continuous capture mode | 0x1
1 | GPIO_INT_ENABLE | TIMER_GPIO_INT_DISABLE | Disable GPIO interrupt capture | 0x0*
|  | TIMER_GPIO_INT_ENABLE | Enable GPIO interrupt capture | 0x1
0 | MODE | TIMER_SHOT_MODE | One shot / multi shot mode | 0x0*
|  | TIMER_FREE_RUN | Free-run mode | 0x1