### BB_RADIOTXRXTIM3

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | RXFLUSHPATHDLY3 | Rx path delay (in us) for coded PHY at 500kbps
22:16 | RW | RFRXTMDA3 | RF Rx test mode delay adjustment for coded PHY at 500kbps
6:0 | RW | TXPATHDLY3 | Rx path delay (in us) for coded PHY at 500kbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | RXFLUSHPATHDLY3 | RXFLUSHPATHDLY3_0 |  | 0x0*
22:16 | RFRXTMDA3 | RFRXTMDA3_0 |  | 0x0*
6:0 | TXPATHDLY3 | TXPATHDLY3_0 |  | 0x0*