### GPIO_MODE

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
15:0 | R | GPIO | GPIO[15:0] mode

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
15:0 | GPIO | GPIO0_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO1_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO2_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO3_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO4_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO5_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO6_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO7_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO8_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO9_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO10_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO11_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO12_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO13_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO14_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO15_IS_NOT_GPIO_MODE | This GPIO is not configured as a CM33 controlled GPIO | 0x0*
|  | GPIO0_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x1
|  | GPIO1_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x2
|  | GPIO2_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x4
|  | GPIO3_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x8
|  | GPIO4_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x10
|  | GPIO5_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x20
|  | GPIO6_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x40
|  | GPIO7_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x80
|  | GPIO8_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x100
|  | GPIO9_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x200
|  | GPIO10_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x400
|  | GPIO11_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x800
|  | GPIO12_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x1000
|  | GPIO13_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x2000
|  | GPIO14_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x4000
|  | GPIO15_IS_GPIO_MODE | This GPIO is configured as a CM33 controlled GPIO | 0x8000