### BB_ACTSCHCNTL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | START_ACT | Request the RW-BLE core to start an event
3:0 | RW | ENTRY_IDX | Indicate the activity scheduler entry index which has to be used when START_ACT is set

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | START_ACT | START_ACT_0 | No action happens if it is written with 0 | 0x0*
|  | START_ACT_1 | Request the RW-BLE Core to start an event | 0x1
3:0 | ENTRY_IDX | ENTRY_IDX_0 |  | 0x0*