### LSAD_MONITOR_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
12 | W | MONITOR_ALARM_CLEAR | Monitoring alarm status bit
9 | W | LSAD_OVERRUN_CLEAR | LSAD Overrun condition
8 | W | LSAD_READY_CLEAR | LSAD new sample Ready status bit
4 | R | MONITOR_ALARM_STAT | Monitoring alarm status bit
1 | R | LSAD_OVERRUN_STAT | LSAD Overrun condition
0 | R | LSAD_READY_STAT | LSAD new sample Ready status bit

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
12 | MONITOR_ALARM_CLEAR | MONITOR_ALARM_CLEAR | Writing a 1 clears the MONITOR Alarm status bit | 0x1
9 | LSAD_OVERRUN_CLEAR | LSAD_OVERRUN_CLEAR | Writing a 1 clears the LSAD Overrun status bit | 0x1
8 | LSAD_READY_CLEAR | LSAD_READY_CLEAR | Writing a 1 clears the LSAD Ready status bit | 0x1
4 | MONITOR_ALARM_STAT | MONITOR_ALARM_FALSE | MONITOR Alarm flag not set | 0x0*
|  | MONITOR_ALARM_TRUE | MONITOR Alarm has been triggered | 0x1
1 | LSAD_OVERRUN_STAT | LSAD_OVERRUN_FALSE | No LSAD Overrun detected | 0x0*
|  | LSAD_OVERRUN_TRUE | LSAD Overrun detected | 0x1
0 | LSAD_READY_STAT | LSAD_READY_FALSE | No new LSAD samples available | 0x0*
|  | LSAD_READY_TRUE | New LSAD samples are ready | 0x1