### LSAD_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
4 | RW | CONTINUOUS_MODE | LSAD continuously sampling the channel selected as interrupt source (LSAD_INT_CH_NUM)
3:0 | RW | FREQ | Defines the sampling frequency of the LSAD channels

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
4 | CONTINUOUS_MODE | LSAD_NORMAL | Normal mode, all 8 channels sampled | 0x0*
|  | LSAD_CONTINUOUS | Continuous mode: only one channel sampled (for test purpose) | 0x1
3:0 | FREQ | LSAD_DISABLE | LSAD disabled | 0x0*
|  | LSAD_PRESCALE_200 | Sample rate is SLOWCLK/200 (low speed mode) | 0x1
|  | LSAD_PRESCALE_400 | Sample rate is SLOWCLK/400 (low speed mode) | 0x2
|  | LSAD_PRESCALE_640 | Sample rate is SLOWCLK/640 (low speed mode) | 0x3
|  | LSAD_PRESCALE_800 | Sample rate is SLOWCLK/800 (low speed mode) | 0x4
|  | LSAD_PRESCALE_1600 | Sample rate is SLOWCLK/1600 (low speed mode) | 0x5
|  | LSAD_PRESCALE_3200 | Sample rate is SLOWCLK/3200 (low speed mode) | 0x6
|  | LSAD_PRESCALE_6400 | Sample rate is SLOWCLK/6400 (low speed mode) | 0x7
|  | LSAD_PRESCALE_20H | Sample rate is SLOWCLK/20 (high speed mode) | 0x8
|  | LSAD_PRESCALE_40H | Sample rate is SLOWCLK/40 (high speed mode) | 0x9
|  | LSAD_PRESCALE_80H | Sample rate is SLOWCLK/80 (high speed mode) | 0xA
|  | LSAD_PRESCALE_128H | Sample rate is SLOWCLK/128 (high speed mode) | 0xB
|  | LSAD_PRESCALE_160H | Sample rate is SLOWCLK/160 (high speed mode) | 0xC
|  | LSAD_PRESCALE_320H | Sample rate is SLOWCLK/320 (high speed mode) | 0xD
|  | LSAD_PRESCALE_640H | Sample rate is SLOWCLK/640 (high speed mode) | 0xE
|  | LSAD_PRESCALE_1280H | Sample rate is SLOWCLK/1280 (high speed mode) | 0xF