### RF_DESER_STATUS

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
7 | R | DESER_STATUS_SIGNAL_RECEIVING | Deserializer enabling
6 | R | DESER_STATUS_SYNC_DETECTED | Sync word detection
5 | R | DESER_STATUS_WAIT_SYNC | Deserializer waiting for the sync word
4 | R | DESER_STATUS_IS_ADDRESS_BR | Received address
3 | R | DESER_STATUS_PKT_LEN_ERR | Packet length
2 | R | DESER_STATUS_ADDRESS_ERR | Address error
1 | R | DESER_STATUS_CRC_ERR | CRC error
0 | R | DESER_STATUS_DESER_FINISH | Deserializer status

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
7 | DESER_STATUS_SIGNAL_RECEIVING | DESER_STATUS_SIGNAL_RECEIVING_DISABLE | Deserializer is disabled | 0x0*
|  | DESER_STATUS_SIGNAL_RECEIVING_ENABLE | Deserializer is enabled | 0x1
6 | DESER_STATUS_SYNC_DETECTED | DESER_STATUS_SYNC_NOT_DETECTED | Sync word (pattern) not detected | 0x0*
|  | DESER_STATUS_SYNC_DETECTED | Sync word (pattern) detected | 0x1
5 | DESER_STATUS_WAIT_SYNC | DESER_STATUS_WAIT_SYNC_NOT_WAITING | Deserializer is not waiting the sync word | 0x0*
|  | DESER_STATUS_WAIT_SYNC_WAITING | Deserializer is waiting the sync word | 0x1
4 | DESER_STATUS_IS_ADDRESS_BR | DESER_STATUS_IS_ADDRESS_BR_DISABLE | The received address is not the broadcast address | 0x0*
|  | DESER_STATUS_IS_ADDRESS_BR_ENABLE | The received address is the broadcast address | 0x1
3 | DESER_STATUS_PKT_LEN_ERR | DESER_STATUS_PKT_LEN_ERR_NO_ERROR | The packet length is shorter than the maximum acceptable packet length | 0x0*
|  | DESER_STATUS_PKT_LEN_ERR_ERROR | The packet length is longer than the maximum acceptable packet length | 0x1
2 | DESER_STATUS_ADDRESS_ERR | DESER_STATUS_ADDRESS_ERR_NO_ERROR | No address error detected | 0x0*
|  | DESER_STATUS_ADDRESS_ERR_ERROR | Address error detected | 0x1
1 | DESER_STATUS_CRC_ERR | DESER_STATUS_CRC_ERR_NO_ERROR | No CRC error detected | 0x0*
|  | DESER_STATUS_CRC_ERR_ERROR | CRC error detected | 0x1
0 | DESER_STATUS_DESER_FINISH | DESER_STATUS_DESER_FINISH_BUSY | Deserializer has not yet finished | 0x0*
|  | DESER_STATUS_DESER_FINISH_IDLE | Deserializer has finished | 0x1