### RF_BIAS_10_12

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
30 | RW | SD_MASH_MASH_DITHER_TYPE | Enable the new dithering scheme
29 | RW | SD_MASH_MASH_ENABLE | Enable the sigma delta mash
28 | RW | SD_MASH_MASH_DITHER | Enable dithering on the sigma delta mash
27:25 | RW | SD_MASH_MASH_ORDER | Order of the sigma delta mash
24 | RW | SD_MASH_MASH_RSTB | Reset of the sigma delta mash (active low)
23:20 | RW | BIAS_12_LNA_AGC_BIAS_3 | LNA bias for AGC level 3
19:16 | RW | BIAS_12_LNA_AGC_BIAS_2 | LNA bias for AGC level 2
15:12 | RW | BIAS_11_LNA_AGC_BIAS_1 | LNA bias for AGC level 1
11:8 | RW | BIAS_11_LNA_AGC_BIAS_0 | LNA bias for AGC level 0
7:4 | RW | BIAS_10_IQ_BB_8 | Peak detector threshold bias 1
3:0 | RW | BIAS_10_IQ_BB_7 | Peak detector threshold bias 2

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
30 | SD_MASH_MASH_DITHER_TYPE | SD_MASH_MASH_DITHER_TYPE_0 | Disable the new dithering scheme | 0x0*
|  | SD_MASH_MASH_DITHER_TYPE_ENABLE | Enable the new dithering scheme | 0x1
29 | SD_MASH_MASH_ENABLE | SD_MASH_MASH_ENABLE_DISABLE | Disable the sigma delta mash | 0x0*
|  | SD_MASH_MASH_ENABLE_ENABLE | Enable the sigma delta mash | 0x1
28 | SD_MASH_MASH_DITHER | SD_MASH_MASH_DITHER_DISABLE | Disable dithering on the sigma delta mash | 0x0
|  | SD_MASH_MASH_DITHER_ENABLE | Enable dithering on the sigma delta mash | 0x1*
27:25 | SD_MASH_MASH_ORDER | SD_MASH_MASH_ORDER_DEFAULT |  | 0x3*
24 | SD_MASH_MASH_RSTB | SD_MASH_MASH_RSTB_RESET | Reset the sigma delta mash | 0x0
|  | SD_MASH_MASH_RSTB_NO_RESET | Do not reset the sigma delta mash | 0x1*
23:20 | BIAS_12_LNA_AGC_BIAS_3 | BIAS_12_LNA_AGC_BIAS_3_DEFAULT |  | 0x6*
19:16 | BIAS_12_LNA_AGC_BIAS_2 | BIAS_12_LNA_AGC_BIAS_2_DEFAULT |  | 0x7*
15:12 | BIAS_11_LNA_AGC_BIAS_1 | BIAS_11_LNA_AGC_BIAS_1_DEFAULT |  | 0x8*
11:8 | BIAS_11_LNA_AGC_BIAS_0 | BIAS_11_LNA_AGC_BIAS_0_DEFAULT |  | 0x9*
7:4 | BIAS_10_IQ_BB_8 | BIAS_10_IQ_BB_8_DEFAULT |  | 0x0*
3:0 | BIAS_10_IQ_BB_7 | BIAS_10_IQ_BB_7_DEFAULT |  | 0x6*