### BB_COEXIFCNTL1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
28:24 | RW | WLCPRXTHR | Determine the threshold for Rx priority setting (apply on ble_rx if WLCRXPRIOMODE equals "10")
20:16 | RW | WLCPTXTHR | Determine the threshold for priority setting (apply on ble_tx if WLCTXPRIOMODE equals "10")
14:8 | RW | WLCPDURATION | Determine how many us the priority information must be maintained (apply on ble_tx and ble_rx if WLCTXPRIOMODE and WLCRXPRIOMODE equal "10")
6:0 | RW | WLCPDELAY | Determine the delay (in us) in Tx/Rx enables rises the time BLE Tx/Rx priority has to be provided (apply on ble_tx and ble_rx if WLCTXPRIOMODE and WLCRXPRIOMODE equal "10")

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
28:24 | WLCPRXTHR | WLCPRXTHR_0 | If ble_pti[3:0] output value is greater than WLCPRXTHR, then Rx BLE priority is considered as high, and must be provided to the WLAN coexistence interface | 0x0*
20:16 | WLCPTXTHR | WLCPTXTHR_0 | If ble_pti[3:0] output value is greater than WLCPTXTHR, then Tx BLE priority is considered as high, and must be provided to the WLAN coexistence interface | 0x0*
14:8 | WLCPDURATION | WLCPDURATION_0 | Note that if WLCPDURATION = 0x00, then Tx/Rx priority levels are maintained till Tx/Rx EN are de-asserted. | 0x0*
6:0 | WLCPDELAY | WLCPDELAY_0 |  | 0x0*