### SYSCTRL_NS_ACCESS_RAM_CFG0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
7:0 | RW | DRAM_ACCESS | Allow Non-Secure to access DRAM[7:0]

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
7:0 | DRAM_ACCESS | NS_CANNOT_ACCESS_DRAM0 | Non-Secure code cannot access the DRAM0 | 0x0*
|  | NS_CANNOT_ACCESS_DRAM1 | Non-Secure code cannot access the DRAM1 | 0x0*
|  | NS_CANNOT_ACCESS_DRAM2 | Non-Secure code cannot access the DRAM2 | 0x0*
|  | NS_CANNOT_ACCESS_DRAM3 | Non-Secure code cannot access the DRAM3 | 0x0*
|  | NS_CANNOT_ACCESS_DRAM4 | Non-Secure code cannot access the DRAM4 | 0x0*
|  | NS_CANNOT_ACCESS_DRAM5 | Non-Secure code cannot access the DRAM5 | 0x0*
|  | NS_CANNOT_ACCESS_DRAM6 | Non-Secure code cannot access the DRAM6 | 0x0*
|  | NS_CANNOT_ACCESS_DRAM7 | Non-Secure code cannot access the DRAM7 | 0x0*
|  | NS_CAN_ACCESS_DRAM0 | Non-Secure code can access the DRAM0 | 0x1
|  | NS_CAN_ACCESS_DRAM1 | Non-Secure code can access the DRAM1 | 0x2
|  | NS_CAN_ACCESS_DRAM2 | Non-Secure code can access the DRAM2 | 0x4
|  | NS_CAN_ACCESS_DRAM3 | Non-Secure code can access the DRAM3 | 0x8
|  | NS_CAN_ACCESS_DRAM4 | Non-Secure code can access the DRAM4 | 0x10
|  | NS_CAN_ACCESS_DRAM5 | Non-Secure code can access the DRAM5 | 0x20
|  | NS_CAN_ACCESS_DRAM6 | Non-Secure code can access the DRAM6 | 0x40
|  | NS_CAN_ACCESS_DRAM7 | Non-Secure code can access the DRAM7 | 0x80