# Ultra-Low Power Data Acquisition Subsystem

Ultra-low power data acquisition (sensor) subsystem hardware abstraction layer.

## Summary

Functions

- Sys_Sensor_SARConfig : Configure the SAR-ADC interface.
- Sys_Sensor_PulseCountConfig : Configure sensor pulse count state.
- Sys_Sensor_StorageConfig : Configure data storage settings.
- Sys_Sensor_DelayConfig : Configure sensor delay clocks and length.
- Sys_Sensor_Enable : Enable the sensor.
- Sys_Sensor_Disable : Disable the sensor.
- Sys_Sensor_TimerReset : The sensor timer counter, the sensor timer enable and the ADC counter are reset.
- Sys_Sensor_CurrentState : Read the current status and delay state of the sensor interface.
- Sys_Sensor_CurrentCountValue : Read the current value of the sensor's main counter.