### GPIO_INT_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
12 | RW | NS_ACCESS | Non-Secure code can access this GPIO_INT (can only be written by a secure code)
11 | RW | DEBOUNCE_ENABLE | Interrupt button debounce filter enable/disable
10:8 | RW | EVENT | Interrupt event configuration
4:0 | RW | SRC | Interrupt input selection

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
12 | NS_ACCESS | NS_CANNOT_ACCESS_GPIO_INT | Non-Secure code cannot access the GPIO_INT | 0x0*
|  | NS_CAN_ACCESS_GPIO_INT | Non-Secure code can access the GPIO_INT | 0x1
11 | DEBOUNCE_ENABLE | GPIO_DEBOUNCE_DISABLE | Button debounce filter disabled | 0x0*
|  | GPIO_DEBOUNCE_ENABLE | Button debounce filter enabled | 0x1
10:8 | EVENT | GPIO_EVENT_NONE | Interrupt not triggered | 0x0*
|  | GPIO_EVENT_HIGH_LEVEL | Interrupt triggered on high state | 0x1
|  | GPIO_EVENT_LOW_LEVEL | Interrupt triggered on low state | 0x2
|  | GPIO_EVENT_RISING_EDGE | Interrupt triggered on rising edge | 0x3
|  | GPIO_EVENT_FALLING_EDGE | Interrupt triggered on falling edge | 0x4
|  | GPIO_EVENT_TRANSITION | Interrupt triggered on any edge | 0x5
4:0 | SRC | GPIO_SRC_GPIO_0 | Select GPIO[0] as source | 0x0*
|  | GPIO_SRC_GPIO_1 | Select GPIO[1] as source | 0x1
|  | GPIO_SRC_GPIO_2 | Select GPIO[2] as source | 0x2
|  | GPIO_SRC_GPIO_3 | Select GPIO[3] as source | 0x3
|  | GPIO_SRC_GPIO_4 | Select GPIO[4] as source | 0x4
|  | GPIO_SRC_GPIO_5 | Select GPIO[5] as source | 0x5
|  | GPIO_SRC_GPIO_6 | Select GPIO[6] as source | 0x6
|  | GPIO_SRC_GPIO_7 | Select GPIO[7] as source | 0x7
|  | GPIO_SRC_GPIO_8 | Select GPIO[8] as source | 0x8
|  | GPIO_SRC_GPIO_9 | Select GPIO[9] as source | 0x9
|  | GPIO_SRC_GPIO_10 | Select GPIO[10] as source | 0xA
|  | GPIO_SRC_GPIO_11 | Select GPIO[11] as source | 0xB
|  | GPIO_SRC_GPIO_12 | Select GPIO[12] as source | 0xC
|  | GPIO_SRC_GPIO_13 | Select GPIO[13] as source | 0xD
|  | GPIO_SRC_GPIO_14 | Select GPIO[14] as source | 0xE
|  | GPIO_SRC_GPIO_15 | Select GPIO[15] as source | 0xF