### NVIC_IABR0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | R | ASCC_PHASE | Set the ASCC_PHASE interrupt as active
30 | R | ASCC_PERIOD | Set the ASCC_PERIOD interrupt as active
29 | R | CC312 | Set the CC312 interrupt as active
28 | R | FPU | Set the FPU interrupt as active
27 | R | LIN0 | Set the LIN0 interrupt as active
26 | R | PCM0_ERROR | Set the PCM0_ERROR interrupt as active
25 | R | PCM0_RX_TX | Set the PCM0_RX_TX interrupt as active
24 | R | UART0_ERROR | Set the UART0_ERROR interrupt as active
23 | R | UART0_TX | Set the UART0_TX interrupt as active
22 | R | UART0_RX | Set the UART0_RX interrupt as active
21 | R | I2C1 | Set the I2C1 interrupt as active
20 | R | I2C0 | Set the I2C0 interrupt as active
19 | R | SPI1_COM | Set the SPI1_COM interrupt as active
18 | R | SPI1_TX | Set the SPI1_TX interrupt as active
17 | R | SPI1_RX | Set the SPI1_RX interrupt as active
16 | R | SPI0_COM | Set the SPI0_COM interrupt as active
15 | R | SPI0_TX | Set the SPI0_TX interrupt as active
14 | R | SPI0_RX | Set the SPI0_RX interrupt as active
13 | R | WATCHDOG | Set the WATCHDOG interrupt as active
12 | R | GPIO3 | Set the GPIO3 interrupt as active
11 | R | GPIO2 | Set the GPIO2 interrupt as active
10 | R | GPIO1 | Set the GPIO1 interrupt as active
9 | R | GPIO0 | Set the GPIO0 interrupt as active
8 | R | FIFO | Set the FIFO interrupt as active
7 | R | TIMER3 | Set the TIMER3 interrupt as active
6 | R | TIMER2 | Set the TIMER2 interrupt as active
5 | R | TIMER1 | Set the TIMER1 interrupt as active
4 | R | TIMER0 | Set the TIMER0 interrupt as active
3 | R | LSAD_MONITOR | Set the LSAD_MONITOR interrupt as active
2 | R | RTC_CLOCK | Set the RTC_CLOCK interrupt as active
1 | R | RTC_ALARM | Set the RTC_ALARM interrupt as active
0 | R | WAKEUP | Set the WAKEUP interrupt as active

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | ASCC_PHASE | NVIC_ASCC_PHASE_INT_ACTIVE | The NVIC_ASCC_PHASE_INT_ACTIVE interrupt is active | 0x1
30 | ASCC_PERIOD | NVIC_ASCC_PERIOD_INT_ACTIVE | The NVIC_ASCC_PERIOD_INT_ACTIVE interrupt is active | 0x1
29 | CC312 | NVIC_CC312_INT_ACTIVE | The NVIC_CC312_INT_ACTIVE interrupt is active | 0x1
28 | FPU | NVIC_FPU_INT_ACTIVE | The NVIC_FPU_INT_ACTIVE interrupt is active | 0x1
27 | LIN0 | NVIC_LIN0_INT_ACTIVE | The NVIC_LIN0_INT_ACTIVE interrupt is active | 0x1
26 | PCM0_ERROR | NVIC_PCM0_ERROR_INT_ACTIVE | The NVIC_PCM0_ERROR_INT_ACTIVE interrupt is active | 0x1
25 | PCM0_RX_TX | NVIC_PCM0_RX_TX_INT_ACTIVE | The NVIC_PCM0_RX_TX_INT_ACTIVE interrupt is active | 0x1
24 | UART0_ERROR | NVIC_UART0_ERROR_INT_ACTIVE | The NVIC_UART0_ERROR_INT_ACTIVE interrupt is active | 0x1
23 | UART0_TX | NVIC_UART0_TX_INT_ACTIVE | The NVIC_UART0_TX_INT_ACTIVE interrupt is active | 0x1
22 | UART0_RX | NVIC_UART0_RX_INT_ACTIVE | The NVIC_UART0_RX_INT_ACTIVE interrupt is active | 0x1
21 | I2C1 | NVIC_I2C1_INT_ACTIVE | The NVIC_I2C1_INT_ACTIVE interrupt is active | 0x1
20 | I2C0 | NVIC_I2C0_INT_ACTIVE | The NVIC_I2C0_INT_ACTIVE interrupt is active | 0x1
19 | SPI1_COM | NVIC_SPI1_COM_INT_ACTIVE | The NVIC_SPI1_COM_INT_ACTIVE interrupt is active | 0x1
18 | SPI1_TX | NVIC_SPI1_TX_INT_ACTIVE | The NVIC_SPI1_TX_INT_ACTIVE interrupt is active | 0x1
17 | SPI1_RX | NVIC_SPI1_RX_INT_ACTIVE | The NVIC_SPI1_RX_INT_ACTIVE interrupt is active | 0x1
16 | SPI0_COM | NVIC_SPI0_COM_INT_ACTIVE | The NVIC_SPI0_COM_INT_ACTIVE interrupt is active | 0x1
15 | SPI0_TX | NVIC_SPI0_TX_INT_ACTIVE | The NVIC_SPI0_TX_INT_ACTIVE interrupt is active | 0x1
14 | SPI0_RX | NVIC_SPI0_RX_INT_ACTIVE | The NVIC_SPI0_RX_INT_ACTIVE interrupt is active | 0x1
13 | WATCHDOG | NVIC_WATCHDOG_INT_ACTIVE | The NVIC_WATCHDOG_INT_ACTIVE interrupt is active | 0x1
12 | GPIO3 | NVIC_GPIO3_INT_ACTIVE | The NVIC_GPIO3_INT_ACTIVE interrupt is active | 0x1
11 | GPIO2 | NVIC_GPIO2_INT_ACTIVE | The NVIC_GPIO2_INT_ACTIVE interrupt is active | 0x1
10 | GPIO1 | NVIC_GPIO1_INT_ACTIVE | The NVIC_GPIO1_INT_ACTIVE interrupt is active | 0x1
9 | GPIO0 | NVIC_GPIO0_INT_ACTIVE | The NVIC_GPIO0_INT_ACTIVE interrupt is active | 0x1
8 | FIFO | NVIC_FIFO_INT_ACTIVE | The NVIC_FIFO_INT_ACTIVE interrupt is active | 0x1
7 | TIMER3 | NVIC_TIMER3_INT_ACTIVE | The NVIC_TIMER3_INT_ACTIVE interrupt is active | 0x1
6 | TIMER2 | NVIC_TIMER2_INT_ACTIVE | The NVIC_TIMER2_INT_ACTIVE interrupt is active | 0x1
5 | TIMER1 | NVIC_TIMER1_INT_ACTIVE | The NVIC_TIMER1_INT_ACTIVE interrupt is active | 0x1
4 | TIMER0 | NVIC_TIMER0_INT_ACTIVE | The NVIC_TIMER0_INT_ACTIVE interrupt is active | 0x1
3 | LSAD_MONITOR | NVIC_LSAD_MONITOR_INT_ACTIVE | The NVIC_LSAD_MONITOR_INT_ACTIVE interrupt is active | 0x1
2 | RTC_CLOCK | NVIC_RTC_CLOCK_INT_ACTIVE | The NVIC_RTC_CLOCK_INT_ACTIVE interrupt is active | 0x1
1 | RTC_ALARM | NVIC_RTC_ALARM_INT_ACTIVE | The NVIC_RTC_ALARM_INT_ACTIVE interrupt is active | 0x1
0 | WAKEUP | NVIC_WAKEUP_INT_ACTIVE | The NVIC_WAKEUP_INT_ACTIVE interrupt is active | 0x1