### RF_REG51

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | FSM_MODE_RM_TX | Remapped register of FSM_MODE
23:16 | RW | PA_PWR_RM | Remapped register of PA_PWR
15:8 | RW | CHANNEL_RM_TX | Remapped register of CHANNEL
7:0 | RW | RATE_TX | Remapped register of BANK

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | FSM_MODE_RM_TX | FSM_MODE_RM_TX_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
23:16 | PA_PWR_RM | PA_PWR_RM_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
15:8 | CHANNEL_RM_TX | CHANNEL_RM_TX_DEFAULT | The remapped registers are accessible over SPI only | 0x0*
7:0 | RATE_TX | RATE_TX_DEFAULT | The remapped registers are accessible over SPI only | 0x0*