### RF_PADS_03

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
28:24 | RW | PAD_CONF_1_PAD_3_CONF | Configuration of GPIO pad 3
20:16 | RW | PAD_CONF_1_PAD_2_CONF | Configuration of GPIO pad 2
12:8 | RW | PAD_CONF_1_PAD_1_CONF | Configuration of GPIO pad 1
4:0 | RW | PAD_CONF_1_PAD_0_CONF | Configuration of GPIO pad 0

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
28:24 | PAD_CONF_1_PAD_3_CONF | PAD_CONF_1_PAD_3_OFF |  | 0x0*
|  | PAD_CONF_1_PAD_3_TEST_MODE |  | 0xF
20:16 | PAD_CONF_1_PAD_2_CONF | PAD_CONF_1_PAD_2_OFF |  | 0x0*
|  | PAD_CONF_1_PAD_2_TEST_MODE |  | 0xF
12:8 | PAD_CONF_1_PAD_1_CONF | PAD_CONF_1_PAD_1_OFF |  | 0x0*
|  | PAD_CONF_1_PAD_1_TEST_MODE |  | 0xF
4:0 | PAD_CONF_1_PAD_0_CONF | PAD_CONF_1_PAD_0_OFF |  | 0x0*
|  | PAD_CONF_1_PAD_0_TEST_MODE |  | 0xF