### ACS_RCOSC_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
26:25 | RW | RC_FSEL | Select RC oscillator frequency
24 | RW | RC_OSC_EN | Enable/Disable the RC Oscillator
23 | RW | RC_FTRIM_FLAG | RC Oscillator Trimming flag
22 | RW | RC_FTRIM_ADJ | Adjust RC oscillator frequency range
21:16 | RW | RC_FTRIM | RC oscillator frequency trimming
15:14 | RW | RC32_VDDLOC_ITRIM | VDDLOC current trimming
13:12 | RW | RC32_VDDLOC_VTRIM | VDDLOC voltage trimming
9 | RW | RC32_VDDLOC_OD_EN | Enable the overdrive of vddloc with VBAT
8 | RW | RC32_OSC_EN | Enable/Disable the 32 kHz RC Oscillator
7 | RW | RC32_TEMP_COMP_EN | Enable/Disable the 32 kHz RC Oscillator
6 | RW | RC32_FTRIM_ADJ | Adjust 32 kHz RC oscillator frequency range
5:0 | RW | RC32_FTRIM | 32 kHz RC oscillator frequency trimming

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
26:25 | RC_FSEL | RC_OSC_3MHZ | The RC Oscillator is at 3 MHz | 0x0*
|  | RC_OSC_12MHZ | The RC Oscillator is at 12 MHz | 0x1
|  | RC_OSC_24MHZ | The RC Oscillator is at 24 MHz | 0x2
|  | RC_OSC_48MHZ | The RC Oscillator is at 48 MHz | 0x3
24 | RC_OSC_EN | RC_OSC_AUTO | The RC Oscillator is in auto mode | 0x0*
|  | RC_OSC_ENABLE | The RC Oscillator is enabled | 0x1
23 | RC_FTRIM_FLAG | RC_OSC_UNCALIBRATED | The oscillators are not calibrated | 0x0*
|  | RC_OSC_CALIBRATED | The oscillators are calibrated | 0x1
22 | RC_FTRIM_ADJ | RC_OSC_RANGE_NOM | The RC Oscillator frequency range is nominal | 0x0*
|  | RC_OSC_RANGE_M15 | The RC Osc higher trim freq is decreased by 15% | 0x1
21:16 | RC_FTRIM | RC_OSC_M48 | -48 % trimming | 0x0
|  | RC_OSC_M46P5 | -46.5% trimming | 0x1
|  | RC_OSC_NOM | Nominal frequency | 0x20*
|  | RC_OSC_P46P5 | +46.5% trimming | 0x3F
9 | RC32_VDDLOC_OD_EN | RC32_OSC_VDDLOC_OD_DISABLE |  | 0x0*
|  | RC32_OSC_VDDLOC_OD_ENABLE |  | 0x1
8 | RC32_OSC_EN | RC32_OSC_DISABLE | The 32kHz RC Oscillator is disabled | 0x0*
|  | RC32_OSC_ENABLE | The 32kHz RC Oscillator is enabled | 0x1
7 | RC32_TEMP_COMP_EN | RC32_TEMP_COMP_DISABLE | The 32kHz RC Oscillator temperature compensation is disabled | 0x0*
|  | RC32_TEMP_COMP_ENABLE | The 32kHz RC Oscillator temperature compensation is enabled | 0x1
6 | RC32_FTRIM_ADJ | RC32_OSC_RANGE_NOM | The 32 kHz RC Oscillator frequency range is nominal | 0x0*
|  | RC32_OSC_RANGE_M25 | The 32 kHz RC Oscillator frequency range is lowered by 25% | 0x1
5:0 | RC32_FTRIM | RC32_OSC_M48 | -48 % trimming | 0x0
|  | RC32_OSC_M46P5 | -46.5% trimming | 0x1
|  | RC32_OSC_NOM | Nominal frequency | 0x20*
|  | RC32_OSC_P46P5 | +46.5% trimming | 0x3F