### FLASH_COPY_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
18 | RW | COMP_ADDR_STEP | Comparator address increment/decrement by 1 or 2
17 | RW | COMP_ADDR_DIR | Comparator address-up or address-down
16 | RW | COMP_MODE | Comparator Mode
9 | RW | COPY_DEST | Destination copier is the CRC or memories
8 | RW | COPY_MODE | Select copier mode (32-bit or 40-bit)
1 | RW | PRIORITY | Copier Priority Configuration
0 | RW | MODE | Copier or Comparator Mode Configuration

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
18 | COMP_ADDR_STEP | COMP_ADDR_STEP_1 | Address increment/decrement by 1 between two reads | 0x0*
|  | COMP_ADDR_STEP_2 | Address increment/decrement by 2 between two reads | 0x1
17 | COMP_ADDR_DIR | COMP_ADDR_DOWN | FLASH_COPIER address count-down | 0x0
|  | COMP_ADDR_UP | FLASH_COPIER address count-up | 0x1*
16 | COMP_MODE | COMP_MODE_CONSTANT | FLASH_DATA[1:0] compare with Flash DOUT | 0x0*
|  | COMP_MODE_CHBK | Odd address compare with FLASH_DATA[1:0], even address compare with inverse FLASH_DATA[1:0] | 0x1
9 | COPY_DEST | COPY_TO_MEM | Copy Flash to memory | 0x0*
|  | COPY_TO_CRC | Copy Flash to CRC | 0x1
8 | COPY_MODE | COPY_TO_32BIT | Copy Flash to 32-bit memory | 0x0*
1 | PRIORITY | FLASH_CM33_PRIORITY | CM33 has priority over Flash Copier | 0x0*
|  | FLASH_COPY_PRIORITY | Flash Copier has priority over CM33 | 0x1
0 | MODE | COPY_MODE | Flash copier mode | 0x0*
|  | COMPARATOR_MODE | Flash comparator mode | 0x1