### GPIO_INT_DEBOUNCE

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
8 | RW | DEBOUNCE_CLK | Interrupt button debounce filter clock
7:0 | RW | DEBOUNCE_COUNT | Interrupt button debounce filter count

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
8 | DEBOUNCE_CLK | GPIO_DEBOUNCE_SLOWCLK_DIV32 | Button debounce filter runs on SLOWCLK divided by 32 | 0x0*
|  | GPIO_DEBOUNCE_SLOWCLK_DIV1024 | Button debounce filter runs on SLOWCLK divided by 1024 | 0x1