### ACS_SDAC_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
2 | RW | SDAC_TO_GPIO7 | GPIO7 drive by SDAC
1 | RW | SDAC_GAIN | Sets the SDAC buffer gain
0 | RW | SDAC_EN | Enable signal for SDAC buffer

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
2 | SDAC_TO_GPIO7 | GPIO7_NOT_DRIVE_BY_SDAC | GPIO[7] not driven by SDAC | 0x0*
|  | GPIO7_DRIVE_BY_SDAC | GPIO[7] drives by SDAC | 0x1
1 | SDAC_GAIN | SDAC_GAIN_X1 | Gain = 1 | 0x0*
|  | SDAC_GAIN_X2 | Gain = 2 | 0x1
0 | SDAC_EN | SDAC_DISABLE | SDAC disabled | 0x0*
|  | SDAC_ENABLE | SDAC enabled | 0x1