### LIN_DLB

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
4 | RW | DELAY | Complete the PID stop bit before sending the first byte
2:0 | RW | DLBT | Number of data bytes to transmit.

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
4 | DELAY | NO_DELAY | No delay added | 0x0*
|  | ADD_DELAY | Finished the Stop bit before sending the byte. | 0x1
2:0 | DLBT | TX_1_BYTE | 1 byte will be transmitted | 0x0*
|  | TX_2_BYTES | 2 bytes will be transmitted | 0x1
|  | TX_3_BYTES | 3 bytes will be transmitted | 0x2
|  | TX_4_BYTES | 4 bytes will be transmitted | 0x3
|  | TX_5_BYTES | 5 bytes will be transmitted | 0x4
|  | TX_6_BYTES | 6 bytes will be transmitted | 0x5
|  | TX_7_BYTES | 7 bytes will be transmitted | 0x6
|  | TX_8_BYTES | 8 bytes will be transmitted | 0x7