# Keil Installation Procedure

Follow the Keil μVision IDE installation instructions provided by Keil. After the Keil IDE is installed, you need to update the SEGGER J-Link software:

1. Go the Start menu and type J-Link DLL Updater V<J-Link_version>, where <J-Link_version> is the version of J-Link recommended for the Keil μVision IDE, and press Enter.
2. Select the Keil MDK-ARM checkbox and click OK.

The RSL15 device is now available in the Keil IDE.