### BB_DIAGCNTL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | DIAG3_EN | Enable diagnostic port 3 output
30:24 | RW | DIAG3 | Selection of the outputs that must be driven to the diagnostic port 3
23 | RW | DIAG2_EN | Enable diagnostic port 2 output
22:16 | RW | DIAG2 | Selection of the outputs that must be driven to the diagnostic port 2
15 | RW | DIAG1_EN | Enable diagnostic port 1 output
14:8 | RW | DIAG1 | Selection of the outputs that must be driven to the diagnostic port 1
7 | RW | DIAG0_EN | Enable diagnostic port 0 output
6:0 | RW | DIAG0 | Selection of the outputs that must be driven to the diagnostic port 1

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | DIAG3_EN | DIAG3_EN_0 | Disable diagnostic port 3 output. All outputs are set to 0x0. | 0x0*
|  | DIAG3_EN_1 | Enable diagnostic port 3 output | 0x1
30:24 | DIAG3 | DIAG3_0 |  | 0x0*
23 | DIAG2_EN | DIAG2_EN_0 | Disable diagnostic port 2 output. All outputs are set to 0x0. | 0x0*
|  | DIAG2_EN_1 | Enable diagnostic port 2 output | 0x1
22:16 | DIAG2 | DIAG2_0 |  | 0x0*
15 | DIAG1_EN | DIAG1_EN_0 | Disable diagnostic port 1 output. All outputs are set to 0x0. | 0x0*
|  | DIAG1_EN_1 | Enable diagnostic port 1 output | 0x1
14:8 | DIAG1 | DIAG1_0 |  | 0x0*
7 | DIAG0_EN | DIAG0_EN_0 | Disable diagnostic port 0 output. All outputs are set to 0x0. | 0x0*
|  | DIAG0_EN_1 | Enable diagnostic port 0 output | 0x1
6:0 | DIAG0 | DIAG0_0 |  | 0x0*