### I2C_ADDR_START

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
7:1 | RW | ADDRESS | I2C address to use for the transaction
0 | RW | READ_WRITE | Select whether a read or a write transaction is started

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
0 | READ_WRITE | I2C_START_WRITE | Start an I2C write transaction | 0x0*
|  | I2C_START_READ | Start an I2C read transaction | 0x1