### BB_DIAGSTAT

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | R | DIAG3STAT | Directly connected to ble_dbg3[7:0] output (debug use only)
23:16 | R | DIAG2STAT | Directly connected to ble_dbg2[7:0] output (debug use only)
15:8 | R | DIAG1STAT | Directly connected to ble_dbg1[7:0] output (debug use only)
7:0 | R | DIAG0STAT | Directly connected to ble_dbg0[7:0] output (debug use only)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | DIAG3STAT | DIAG3STAT_0 |  | 0x0*
23:16 | DIAG2STAT | DIAG2STAT_0 |  | 0x0*
15:8 | DIAG1STAT | DIAG1STAT_0 |  | 0x0*
7:0 | DIAG0STAT | DIAG0STAT_0 |  | 0x0*