### SYSCTRL_MEM_POWER_STARTUP

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
17:16 | RW | BB_DRAM_STARTUP | Baseband DRAM[1:0] power startup control
15:8 | RW | DRAM_STARTUP | DRAM[7:0] power startup control
1 | RW | FLASH_STARTUP | Flash[0:0] power startup control
0 | RW | PROM_STARTUP | PROM power startup control

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
17:16 | BB_DRAM_STARTUP | BB_DRAM0_POWER_OFF | Baseband DRAM0 startup disabled | 0x0
|  | BB_DRAM1_POWER_OFF | Baseband DRAM1 startup disabled | 0x0
|  | BB_DRAM0_POWER_STARTUP | Baseband DRAM0 startup enabled | 0x1
|  | BB_DRAM1_POWER_STARTUP | Baseband DRAM1 startup enabled | 0x2
15:8 | DRAM_STARTUP | DRAM0_POWER_OFF | DRAM0 startup disabled | 0x0
|  | DRAM1_POWER_OFF | DRAM1 startup disabled | 0x0
|  | DRAM2_POWER_OFF | DRAM2 startup disabled | 0x0
|  | DRAM3_POWER_OFF | DRAM3 startup disabled | 0x0
|  | DRAM4_POWER_OFF | DRAM4 startup disabled | 0x0
|  | DRAM5_POWER_OFF | DRAM5 startup disabled | 0x0
|  | DRAM6_POWER_OFF | DRAM6 startup disabled | 0x0
|  | DRAM7_POWER_OFF | DRAM7 startup disabled | 0x0
|  | DRAM0_POWER_STARTUP | DRAM0 startup enabled | 0x1
|  | DRAM1_POWER_STARTUP | DRAM1 startup enabled | 0x2
|  | DRAM2_POWER_STARTUP | DRAM2 startup enabled | 0x4
|  | DRAM3_POWER_STARTUP | DRAM3 startup enabled | 0x8
|  | DRAM4_POWER_STARTUP | DRAM4 startup enabled | 0x10
|  | DRAM5_POWER_STARTUP | DRAM5 startup enabled | 0x20
|  | DRAM6_POWER_STARTUP | DRAM6 startup enabled | 0x40
|  | DRAM7_POWER_STARTUP | DRAM7 startup enabled | 0x80
1 | FLASH_STARTUP | FLASH0_POWER_OFF | FLASH0 startup disabled | 0x0*
|  | FLASH0_POWER_STARTUP | FLASH0 startup enabled | 0x1
0 | PROM_STARTUP | PROM_POWER_OFF | PROM startup disabled | 0x0
|  | PROM_POWER_STARTUP | PROM startup enabled | 0x1*