### ACS_WAKEUP_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
27 | R | RTC_OVERFLOW_WAKEUP | Indicate if RTC overflow has triggered a wake-up event
26 | R | RTC_CLOCK_WAKEUP | Indicate if RTC clock has triggered a wake-up event
25 | R | RTC_ALARM_WAKEUP | Indicate if RTC alarm has triggered a wake-up event
24 | R | THRESHOLD_WAKEUP | Indicate if the sensor interface threshold has triggered a wake-up event
23 | R | FIFO_FULL_WAKEUP | Indicate if the sensor interface FIFO has triggered a wake-up event
22 | R | ACOMP_WAKEUP | Indicate if ACOMP has triggered a wake-up event
21 | R | DCDC_OVERLOAD_WAKEUP | Indicate if DCDC overload has triggered a wake-up event
20 | R | BB_TIMER_WAKEUP | Indicate if baseband timer has triggered a wake-up event
19 | R | GPIO3_WAKEUP | Indicate if GPIO3 has triggered a wake-up event
18 | R | GPIO2_WAKEUP | Indicate if GPIO2 has triggered a wake-up event
17 | R | GPIO1_WAKEUP | Indicate if GPIO1 has triggered a wake-up event
16 | R | GPIO0_WAKEUP | Indicate if GPIO0 has triggered a wake-up event
11 | W | THRESHOLD_WAKEUP_CLEAR | Reset the sticky WAKEUP_THRESHOLD_EVENT flag
10 | W | FIFO_FULL_WAKEUP_CLEAR | Reset the sticky WAKEUP_FIFO_FULL_EVENT flag
9 | W | ACOMP_WAKEUP_CLEAR | Reset the sticky WAKEUP_ACOMP_EVENT flag
8 | W | DCDC_OVERLOAD_WAKEUP_CLEAR | Reset the sticky WAKEUP_DCDC_OVERLOAD flag
7 | W | RTC_OVERFLOW_WAKEUP_CLEAR | Reset the sticky WAKEUP_RTC_OVERFLOW_EVENT flag
6 | W | RTC_CLOCK_WAKEUP_CLEAR | Reset the sticky WAKEUP_RTC_CLOCK_EVENT flag
5 | W | RTC_ALARM_WAKEUP_CLEAR | Reset the sticky WAKEUP_RTC_ALARM_EVENT flag
4 | W | BB_TIMER_WAKEUP_CLEAR | Reset the sticky WAKEUP_BB_TIMER_EVENT flag
3 | W | GPIO3_WAKEUP_CLEAR | Reset the sticky WAKEUP_GPIO3_EVENT flag
2 | W | GPIO2_WAKEUP_CLEAR | Reset the sticky WAKEUP_GPIO2_EVENT flag
1 | W | GPIO1_WAKEUP_CLEAR | Reset the sticky WAKEUP_GPIO1_EVENT flag
0 | W | GPIO0_WAKEUP_CLEAR | Reset the sticky WAKEUP_GPIO0_EVENT flag

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
27 | RTC_OVERFLOW_WAKEUP | WAKEUP_RTC_OVERFLOW_EVENT_NOT_SET | RTC overflow has not triggered a wake-up event | 0x0*
|  | WAKEUP_RTC_OVERFLOW_EVENT_SET | RTC overflow has triggered a wake-up event at least once | 0x1
26 | RTC_CLOCK_WAKEUP | WAKEUP_RTC_CLOCK_EVENT_NOT_SET | RTC clock has not triggered a wake-up event | 0x0*
|  | WAKEUP_RTC_CLOCK_EVENT_SET | RTC clock has triggered a wake-up event at least once | 0x1
25 | RTC_ALARM_WAKEUP | WAKEUP_RTC_ALARM_EVENT_NOT_SET | RTC alarm has not triggered a wake-up event | 0x0*
|  | WAKEUP_RTC_ALARM_EVENT_SET | RTC alarm has triggered a wake-up event at least once | 0x1
24 | THRESHOLD_WAKEUP | WAKEUP_THRESHOLD_EVENT_NOT_SET | The ULP data acquisition subsystem threshold has not triggered a wake-up event | 0x0*
|  | WAKEUP_THRESHOLD_EVENT_SET | The ULP data acquisition subsystem threshold has triggered a wake-up event at least once | 0x1
23 | FIFO_FULL_WAKEUP | WAKEUP_FIFO_FULL_EVENT_NOT_SET | The ULP data acquisition subsystem FIFO has not triggered a wake-up event | 0x0*
|  | WAKEUP_FIFO_FULL_EVENT_SET | The ULP data acquisition subsystem FIFO has triggered a wake-up event at least once | 0x1
22 | ACOMP_WAKEUP | WAKEUP_ACOMP_EVENT_NOT_SET | The ACOMP has not triggered a wake-up event | 0x0*
|  | WAKEUP_ACOMP_EVENT_SET | The ACOMP has triggered a wake-up event at least once | 0x1
21 | DCDC_OVERLOAD_WAKEUP | WAKEUP_DCDC_OVERLOAD_EVENT_NOT_SET | DCDC overload has not triggered a wake-up event | 0x0*
|  | WAKEUP_DCDC_OVERLOAD_EVENT_SET | DCDC overload has triggered a wake-up event at least once | 0x1
20 | BB_TIMER_WAKEUP | WAKEUP_BB_TIMER_EVENT_NOT_SET | BB timer has not triggered a wake-up event | 0x0*
|  | WAKEUP_BB_TIMER_EVENT_SET | BB timer has triggered a wake-up event at least once | 0x1
19 | GPIO3_WAKEUP | WAKEUP_GPIO3_EVENT_NOT_SET | GPIO3 has not triggered a wake-up event | 0x0*
|  | WAKEUP_GPIO3_EVENT_SET | GPIO3 has triggered a wake-up event at least once | 0x1
18 | GPIO2_WAKEUP | WAKEUP_GPIO2_EVENT_NOT_SET | GPIO2 has not triggered a wake-up event | 0x0*
|  | WAKEUP_GPIO2_EVENT_SET | GPIO2 has triggered a wake-up event at least once | 0x1
17 | GPIO1_WAKEUP | WAKEUP_GPIO1_EVENT_NOT_SET | GPIO1 has not triggered a wake-up event | 0x0*
|  | WAKEUP_GPIO1_EVENT_SET | GPIO1 has triggered a wake-up event at least once | 0x1
16 | GPIO0_WAKEUP | WAKEUP_GPIO0_EVENT_NOT_SET | GPIO0 has not triggered a wake-up event | 0x0*
|  | WAKEUP_GPIO0_EVENT_SET | GPIO0 has triggered a wake-up event at least once | 0x1
11 | THRESHOLD_WAKEUP_CLEAR | THRESHOLD_FULL_EVENT_CLEAR | Reset the sticky WAKEUP_THRESHOLD_EVENT flag | 0x1
10 | FIFO_FULL_WAKEUP_CLEAR | WAKEUP_FIFO_FULL_EVENT_CLEAR | Reset the sticky WAKEUP_FIFO_FULL_EVENT flag | 0x1
9 | ACOMP_WAKEUP_CLEAR | WAKEUP_ACOMP_EVENT_CLEAR | Reset the sticky WAKEUP_ACOMP_EVENT flag | 0x1
8 | DCDC_OVERLOAD_WAKEUP_CLEAR | WAKEUP_DCDC_OVERLOAD_EVENT_CLEAR | Reset the sticky WAKEUP_DCDC_OVERLOAD flag | 0x1
7 | RTC_OVERFLOW_WAKEUP_CLEAR | WAKEUP_RTC_OVERFLOW_EVENT_CLEAR | Reset the sticky WAKEUP_RTC_OVERFLOW_EVENT flag | 0x1
6 | RTC_CLOCK_WAKEUP_CLEAR | WAKEUP_RTC_CLOCK_EVENT_CLEAR | Reset the sticky WAKEUP_RTC_CLOCK_EVENT flag | 0x1
5 | RTC_ALARM_WAKEUP_CLEAR | WAKEUP_RTC_ALARM_EVENT_CLEAR | Reset the sticky WAKEUP_RTC_ALARM_EVENT flag | 0x1
4 | BB_TIMER_WAKEUP_CLEAR | WAKEUP_BB_TIMER_CLEAR | Reset the sticky WAKEUP_BB_TIMER_EVENT flag | 0x1
3 | GPIO3_WAKEUP_CLEAR | WAKEUP_GPIO3_EVENT_CLEAR | Reset the sticky WAKEUP_GPIO3_EVENT flag | 0x1
2 | GPIO2_WAKEUP_CLEAR | WAKEUP_GPIO2_EVENT_CLEAR | Reset the sticky WAKEUP_GPIO2_EVENT flag | 0x1
1 | GPIO1_WAKEUP_CLEAR | WAKEUP_GPIO1_EVENT_CLEAR | Reset the sticky WAKEUP_GPIO1_EVENT flag | 0x1
0 | GPIO0_WAKEUP_CLEAR | WAKEUP_GPIO0_EVENT_CLEAR | Reset the sticky WAKEUP_GPIO0_EVENT flag | 0x1