### RF_AGC_LUT5

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
26:25 | RW | IEEE802154_OPTS_CNT_LIM_802154 | Set the number of samples to wait before increasing the threshold
24:22 | RW | IEEE802154_OPTS_CNT_OK_INC_802154 | Set the increment to the counter that indicates that the correlators peaks are coherent
21 | RW | IEEE802154_OPTS_USE_OS_802154 | Enable the new algorithm working in the oversampled domain for the demodulation of the IEEE 802.15.4 protocol
20 | RW | IEEE802154_OPTS_EN_DW_TEST | Tx data-whitening before the convolutional code block
18:16 | RW | IEEE802154_OPTS_C2B_THR | Threshold of the chip2bit correlator of the IEEE 802.15.4 protocol
13:12 | RW | DATA_STREAMS_BER_CLK_MODE | Set the clock output mode for BER mode or RW mode
10 | RW | DATA_STREAMS_RX_DATA_NOT_SAMPLED | Signal rx_data in test modes sampling
9 | RW | DATA_STREAMS_PHASE_GREY | Phase signal encoding
8 | RW | DATA_STREAMS_TX_IN_CLK_TOGGLE | Input clock
3:0 | RW | AGC_LUT_5_AGC_LEVEL_11_HI | AGC values level 11 (MSB)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
26:25 | IEEE802154_OPTS_CNT_LIM_802154 | IEEE802154_OPTS_CNT_LIM_802154_DEFAULT |  | 0x2*
24:22 | IEEE802154_OPTS_CNT_OK_INC_802154 | IEEE802154_OPTS_CNT_OK_INC_802154_DEFAULT |  | 0x4*
21 | IEEE802154_OPTS_USE_OS_802154 | IEEE802154_OPTS_USE_OS_802154_DISABLE | Disable the Tx data-whitening | 0x0
|  | IEEE802154_OPTS_USE_OS_802154_ENABLE | Enable the Tx data-whitening | 0x1*
20 | IEEE802154_OPTS_EN_DW_TEST | IEEE802154_OPTS_EN_DW_TEST_DISABLE | Disable the Tx data-whitening | 0x0*
|  | IEEE802154_OPTS_EN_DW_TEST_ENABLE | Enable the Tx data-whitening | 0x1
18:16 | IEEE802154_OPTS_C2B_THR | IEEE802154_OPTS_C2B_THR_DEFAULT |  | 0x4*
13:12 | DATA_STREAMS_BER_CLK_MODE | DATA_STREAMS_BER_CLK_MODE_FALLING | data change on falling edge | 0x0*
|  | DATA_STREAMS_BER_CLK_MODE_RISING | Data change on rising edge | 0x1
|  | DATA_STREAMS_BER_CLK_MODE_TOGGLE | Clock signal is a toggled signal | 0x2
|  | DATA_STREAMS_BER_CLK_MODE_RECOVERY | Enable signal from clock recovery | 0x3
10 | DATA_STREAMS_RX_DATA_NOT_SAMPLED | DATA_STREAMS_RX_DATA_NOT_SAMPLED_DISABLE | The signal rx_data in test modes is sampled | 0x0*
|  | DATA_STREAMS_RX_DATA_NOT_SAMPLED_ENABLE | The signal rx_data in test modes is not sampled | 0x1
9 | DATA_STREAMS_PHASE_GREY | DATA_STREAMS_PHASE_GREY_DISABLE | The phase signal on the test bus is not grey encoded | 0x0*
|  | DATA_STREAMS_PHASE_GREY_ENABLE | The phase signal on the test bus is grey encoded | 0x1
8 | DATA_STREAMS_TX_IN_CLK_TOGGLE | DATA_STREAMS_TX_IN_CLK_TOGGLE_DISABLE | Input clock is not a toggling signal | 0x0*
|  | DATA_STREAMS_TX_IN_CLK_TOGGLE_ENABLE | input clock is a toggling signal | 0x1
3:0 | AGC_LUT_5_AGC_LEVEL_11_HI | AGC_LUT_5_AGC_LEVEL_11_HI_DEFAULT |  | 0xE*