### BB_BLEMPRIO0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | BLEM7 | Set priority value for passive scanning
27:24 | RW | BLEM6 | Set priority value for non-connectable advertising
23:20 | RW | BLEM5 | Set priority value for connectable advertising BLE message
19:16 | RW | BLEM4 | Set priority value for active scanning BLE message
15:12 | RW | BLEM3 | Set priority value for initiating (scanning) BLE message
11:8 | RW | BLEM2 | Set priority value for data channel transmission BLE message
7:4 | RW | BLEM1 | Set priority value for LLCP BLE message
3:0 | RW | BLEM0 | Set priority value for initiating (connection request response) BLE message

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | BLEM7 | BLEM7_3 |  | 0x3*
27:24 | BLEM6 | BLEM6_4 |  | 0x4*
23:20 | BLEM5 | BLEM5_8 |  | 0x8*
19:16 | BLEM4 | BLEM4_9 |  | 0x9*
15:12 | BLEM3 | BLEM3_10 |  | 0xA*
11:8 | BLEM2 | BLEM2_13 |  | 0xD*
7:4 | BLEM1 | BLEM1_14 |  | 0xE*
3:0 | BLEM0 | BLEM0_15 |  | 0xF*