### BB_INTCNTL0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
16 | RW | ERRORINTMSK | Error interrupt mask
6 | RW | ISORXINTMSK | Isochronous channel Rx interrupt mask
5 | RW | ISOTXINTMSK | Isochronous channel Tx interrupt mask
4 | RW | RXINTMSK | Rx interrupt mask
3 | RW | TXINTMSK | Tx interrupt mask
2 | RW | SKIPEVTINTMSK | Skipped event interrupt mask
1 | RW | ENDEVTINTMSK | End of event interrupt mask
0 | RW | STARTEVTINTMSK | Start of event interrupt mask

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
16 | ERRORINTMSK | ERRORINTMSK_0 | Interrupt not generated | 0x0*
|  | ERRORINTMSK_1 | Interrupt generated | 0x1
6 | ISORXINTMSK | ISORXINTMSK_0 | Interrupt not reported in FIFO IRQ | 0x0*
|  | ISORXINTMSK_1 | Interrupt reported in FIFO IRQ | 0x1
5 | ISOTXINTMSK | ISOTXINTMSK_0 | Interrupt not reported in FIFO IRQ | 0x0*
|  | ISOTXINTMSK_1 | Interrupt reported in FIFO IRQ | 0x1
4 | RXINTMSK | RXINTMSK_0 | Interrupt not reported in FIFO IRQ | 0x0*
|  | RXINTMSK_1 | Interrupt reported in FIFO IRQ | 0x1
3 | TXINTMSK | TXINTMSK_0 | Interrupt not reported in FIFO IRQ | 0x0*
|  | TXINTMSK_1 | Interrupt reported in FIFO IRQ | 0x1
2 | SKIPEVTINTMSK | SKIPEVTINTMSK_0 | Interrupt not reported in FIFO IRQ | 0x0*
|  | SKIPEVTINTMSK1 | Interrupt reported in FIFO IRQ | 0x1
1 | ENDEVTINTMSK | ENDEVTINTMSK_0 | Interrupt not reported in FIFO IRQ | 0x0
|  | ENDEVTINTMSK_1 | Interrupt reported in FIFO IRQ | 0x1*
0 | STARTEVTINTMSK | STARTEVTINTMSK_0 | Interrupt not reported in FIFO IRQ | 0x0
|  | STARTEVTINTMSK_1 | Interrupt reported in FIFO IRQ | 0x1*