# Integrating FOTA Into Your Application

This topic shows how to modify an existing sample application to make it capable of receiving FOTA updates. We start with the ble_peripheral_direction_finding application, and walk you step-by-step through all the required project configurations and firmware changes. Then we show how to perform a FOTA update to confirm that the integration has been executed successfully.

NOTE: This information refers to the general FOTA usage. For information on performing a secure FOTA update, refer to the instructions and examples in the secure_blinky_fota sample application’s readme file.

For more information about this topic, see: