### SYSCTRL_ACCESS_ERROR

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
16 | W | ACCESS_ERROR_CLEAR | Write a 1 to clear the access error flags
12 | R | CC312_MEM_ERROR | CC312 memory error flag
10 | R | DMA_PERIPH_ERROR | DMA peripheral access error flag
9 | R | DMA_MEM_ERROR | DMA memory error flag
8 | R | BB_MEM_ERROR | Baseband memory error flag
0 | R | FLASH_COPIER_MEM_ERROR | FLASH[0:0] copier memory error flag

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
16 | ACCESS_ERROR_CLEAR | SYSCTRL_ACCESS_ERROR_CLEAR | Clear the access error flags | 0x1
12 | CC312_MEM_ERROR | CC312_MEM_NO_ERROR_DETECTED | No CC312 memory error detected | 0x0*
|  | CC312_MEM_ERROR_DETECTED | CC312 has accessed an isolated memory | 0x1
10 | DMA_PERIPH_ERROR | DMA_PERIPH_NO_ERROR_DETECTED | No DMA peripheral access error detected | 0x0*
|  | DMA_PERIPH_ERROR_DETECTED | DMA received a peripheral access error | 0x1
9 | DMA_MEM_ERROR | DMA_MEM_NO_ERROR_DETECTED | No DMA memory error detected | 0x0*
|  | DMA_MEM_ERROR_DETECTED | DMA has accessed an isolated memory | 0x1
8 | BB_MEM_ERROR | BB_MEM_NO_ERROR_DETECTED | No baseband memory error detected | 0x0*
|  | BB_MEM_ERROR_DETECTED | Baseband has accessed an isolated memory | 0x1
0 | FLASH_COPIER_MEM_ERROR | FLASH0_COPIER_MEM_NO_ERROR_DETECTED | No FLASH copier memory error detected | 0x0*
|  | FLASH0_COPIER_MEM_ERROR_DETECTED | FLASH0 copier has accessed an isolated memory | 0x1