### RF_CENTER_FREQ

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31 | RW | CENTER_FREQ_ADAPT_CFREQ | Frequency adaptation between Tx and Rx modes
30 | RW | CENTER_FREQ_RX_DIV_5_N6 | Ratio of the PLL reference between Tx and Rx modes
29:0 | RW | CENTER_FREQ_CENTER_FREQUENCY | Set the center frequency

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31 | CENTER_FREQ_ADAPT_CFREQ | CENTER_FREQ_ADAPT_CFREQ_DISABLE | Do not adapt frequency between Tx and Rx | 0x0
|  | CENTER_FREQ_ADAPT_CFREQ_ENABLE | Automatically adapt frequency between Tx and Rx | 0x1*
30 | CENTER_FREQ_RX_DIV_5_N6 | CENTER_FREQ_RX_DIV_5_N6_DISABLE | The ratio of the PLL reference between Tx and Rx is 6 instead of 5 | 0x0*
|  | CENTER_FREQ_RX_DIV_5_N6_ENABLE | The ratio of the PLL reference between Tx and Rx is 5 instead of 6 | 0x1
29:0 | CENTER_FREQ_CENTER_FREQUENCY | CENTER_FREQ_CENTER_FREQUENCY_DEFAULT |  | 0x215C71B*