### SYSCTRL_MEM_RETENTION_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
17:16 | RW | BB_DRAM_RETENTION | Baseband DRAM[1:0] retention configuration
15:8 | RW | DRAM_RETENTION | DRAM[7:0] retention configuration

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
17:16 | BB_DRAM_RETENTION | BB_DRAM0_NORMAL_MODE | Baseband DRAM0 normal mode | 0x0
|  | BB_DRAM1_NORMAL_MODE | Baseband DRAM1 normal mode | 0x0
|  | BB_DRAM0_RETENTION_MODE | Baseband DRAM0 retention mode | 0x1
|  | BB_DRAM1_RETENTION_MODE | Baseband DRAM1 retention mode | 0x2
15:8 | DRAM_RETENTION | DRAM0_NORMAL_MODE | DRAM0 normal mode | 0x0
|  | DRAM1_NORMAL_MODE | DRAM1 normal mode | 0x0
|  | DRAM2_NORMAL_MODE | DRAM2 normal mode | 0x0
|  | DRAM3_NORMAL_MODE | DRAM3 normal mode | 0x0
|  | DRAM4_NORMAL_MODE | DRAM4 normal mode | 0x0
|  | DRAM5_NORMAL_MODE | DRAM5 normal mode | 0x0
|  | DRAM6_NORMAL_MODE | DRAM6 normal mode | 0x0
|  | DRAM7_NORMAL_MODE | DRAM7 normal mode | 0x0
|  | DRAM0_RETENTION_MODE | DRAM0 retention mode | 0x1
|  | DRAM1_RETENTION_MODE | DRAM1 retention mode | 0x2
|  | DRAM2_RETENTION_MODE | DRAM2 retention mode | 0x4
|  | DRAM3_RETENTION_MODE | DRAM3 retention mode | 0x8
|  | DRAM4_RETENTION_MODE | DRAM4 retention mode | 0x10
|  | DRAM5_RETENTION_MODE | DRAM5 retention mode | 0x20
|  | DRAM6_RETENTION_MODE | DRAM6 retention mode | 0x40
|  | DRAM7_RETENTION_MODE | DRAM7 retention mode | 0x80