### BBIF_COEX_INT_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
7:6 | RW | EVENT_IN_PROCESS | EVENT_IN_PROCESS event interrupt configuration
5:4 | RW | BLE_IN_PROCESS | BLE_IN_PROCESS event interrupt configuration
3:2 | RW | BLE_TX | BLE_TX event interrupt configuration
1:0 | RW | BLE_RX | BLE_RX event interrupt configuration

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
7:6 | EVENT_IN_PROCESS | EVENT_IN_PROCESS_NONE | Interrupt not triggered | 0x0*
|  | EVENT_IN_PROCESS_RISING_EDGE | Interrupt triggered on rising edge | 0x1
|  | EVENT_IN_PROCESS_FALLING_EDGE | Interrupt triggered on falling edge | 0x2
|  | EVENT_IN_PROCESS_TRANSITION | Interrupt triggered on any edge | 0x3
5:4 | BLE_IN_PROCESS | BLE_IN_PROCESS_NONE | Interrupt not triggered | 0x0*
|  | BLE_IN_PROCESS_RISING_EDGE | Interrupt triggered on rising edge | 0x1
|  | BLE_IN_PROCESS_FALLING_EDGE | Interrupt triggered on falling edge | 0x2
|  | BLE_IN_PROCESS_TRANSITION | Interrupt triggered on any edge | 0x3
3:2 | BLE_TX | BLE_TX_NONE | Interrupt not triggered | 0x0*
|  | BLE_TX_RISING_EDGE | Interrupt triggered on rising edge | 0x1
|  | BLE_TX_FALLING_EDGE | Interrupt triggered on falling edge | 0x2
|  | BLE_TX_TRANSITION | Interrupt triggered on any edge | 0x3
1:0 | BLE_RX | BLE_RX_NONE | Interrupt not triggered | 0x0*
|  | BLE_RX_RISING_EDGE | Interrupt triggered on rising edge | 0x1
|  | BLE_RX_FALLING_EDGE | Interrupt triggered on falling edge | 0x2
|  | BLE_RX_TRANSITION | Interrupt triggered on any edge | 0x3