### ACS_WAKEUP_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
18:16 | RW | DELAY | Delay from VDDD ready to digital clock enable (power of 2)
11 | RW | DCDC_OVERLOAD_EN | Enable / Disable the Wake-up functionality on the DCDC overload flag
9 | RW | FIFO_FULL_EN | Enable the wake-up on full FIFO
8 | RW | RTC_OVERFLOW_EN | Enable / Disable the Wake-up functionality on RTC overflow flag
7 | RW | GPIO3_POL | Wake-up polarity on the GPIO3 pad
6 | RW | GPIO2_POL | Wake-up polarity on the GPIO2 pad
5 | RW | GPIO1_POL | Wake-up polarity on the GPIO1 pad
4 | RW | GPIO0_POL | Wake-up polarity on the GPIO0 pad
3 | RW | GPIO3_EN | Enable the wake-up functionality on the GPIO3 pad
2 | RW | GPIO2_EN | Enable the wake-up functionality on the GPIO2 pad
1 | RW | GPIO1_EN | Enable the wake-up functionality on the GPIO1 pad
0 | RW | GPIO0_EN | Enable the wake-up functionality on the GPIO0 pad

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
18:16 | DELAY | WAKEUP_DELAY_1 | Wait for 1 32kHz clock cycle | 0x0
|  | WAKEUP_DELAY_2 | Wait for 2 32kHz clock cycles | 0x1
|  | WAKEUP_DELAY_4 | Wait for 4 32kHz clock cycles | 0x2
|  | WAKEUP_DELAY_8 | Wait for 8 32kHz clock cycles | 0x3
|  | WAKEUP_DELAY_16 | Wait for 16 32kHz clock cycles | 0x4*
|  | WAKEUP_DELAY_32 | Wait for 32 32kHz clock cycles | 0x5
|  | WAKEUP_DELAY_64 | Wait for 64 32kHz clock cycles | 0x6
|  | WAKEUP_DELAY_128 | Wait for 128 32kHz clock cycles | 0x7
11 | DCDC_OVERLOAD_EN | WAKEUP_DCDC_OVERLOAD_DISABLE | Disable the wake-up functionality on the DCDC overload flag | 0x0*
|  | WAKEUP_DCDC_OVERLOAD_ENABLE | Enable the wake-up functionality on the DCDC overload flag | 0x1
9 | FIFO_FULL_EN | WAKEUP_FIFO_DISABLE | Disable the wake-up functionality on the ULP data acquisition subsystem FIFO | 0x0*
|  | WAKEUP_FIFO_ENABLE | Enable the wake-up functionality on the ULP data acquisition subsystem FIFO | 0x1
8 | RTC_OVERFLOW_EN | WAKEUP_RTC_OVERFLOW_DISABLE | Disable the wake-up functionality on the RTC overflow flag | 0x0*
|  | WAKEUP_RTC_OVERFLOW_ENABLE | Enable the wake-up functionality on the RTC overflow flag | 0x1
7 | GPIO3_POL | WAKEUP_GPIO3_RISING | Wake-up on the GPIO3 rising edge | 0x0*
|  | WAKEUP_GPIO3_FALLING | Wake-up on the GPIO3 falling edge | 0x1
6 | GPIO2_POL | WAKEUP_GPIO2_RISING | Wake-up on the GPIO2 rising edge | 0x0*
|  | WAKEUP_GPIO2_FALLING | Wake-up on the GPIO2 falling edge | 0x1
5 | GPIO1_POL | WAKEUP_GPIO1_RISING | Wake-up on the GPIO1 rising edge | 0x0*
|  | WAKEUP_GPIO1_FALLING | Wake-up on the GPIO1 falling edge | 0x1
4 | GPIO0_POL | WAKEUP_GPIO0_RISING | Wake-up on the GPIO0 rising edge | 0x0*
|  | WAKEUP_GPIO0_FALLING | Wake-up on the GPIO0 falling edge | 0x1
3 | GPIO3_EN | WAKEUP_GPIO3_DISABLE | Disable the wake-up functionality on the GPIO3 pad | 0x0*
|  | WAKEUP_GPIO3_ENABLE | Enable the wake-up functionality on the GPIO3 pad | 0x1
2 | GPIO2_EN | WAKEUP_GPIO2_DISABLE | Disable the wake-up functionality on the GPIO2 pad | 0x0*
|  | WAKEUP_GPIO2_ENABLE | Enable the wake-up functionality on the GPIO2 pad | 0x1
1 | GPIO1_EN | WAKEUP_GPIO1_DISABLE | Disable the wake-up functionality on the GPIO1 pad | 0x0*
|  | WAKEUP_GPIO1_ENABLE | Enable the wake-up functionality on the GPIO1 pad | 0x1
0 | GPIO0_EN | WAKEUP_GPIO0_DISABLE | Disable the wake-up functionality on the GPIO0 pad | 0x0*
|  | WAKEUP_GPIO0_ENABLE | Enable the wake-up functionality on the GPIO0 pad | 0x1