### RF_FEI

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:16 | R | FEI_PKT_FEI_PKT | Frequency error indicator sampled during the packet reception
15:0 | R | FEI_FEI_OUT | Frequency error indicator

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:16 | FEI_PKT_FEI_PKT | FEI_PKT_FEI_PKT_DEFAULT |  | 0x0*
15:0 | FEI_FEI_OUT | FEI_FEI_OUT_DEFAULT |  | 0x0*