### TIMER_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
8 | R | BUSY | Indicate if the timer is active or not
1 | W | START | Start or restart the timer
0 | W | STOP | Stop the timer

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
8 | BUSY | TIMER_INACTIVE | The timer is inactive | 0x0*
|  | TIMER_ACTIVE | The timer is active | 0x1
1 | START | TIMER_START | Writing a 1 starts or restarts the timer | 0x1
0 | STOP | TIMER_STOP | Writing a 1 stops the timer | 0x1