### RF_REG02

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
25:24 | RW | DATARATE_OFFSET_DR_LIMIT | Set the data-rate recovery limits
23:16 | RW | DATARATE_OFFSET_DATARATE_OFFSET | Data-rate offset
15:8 | RW | TAU_DATARATE_RECOV_TAU_DATARATE_RECOV | Time constant of the data-rate recovery
7:0 | RW | TAU_CLK_RECOV_TAU_CLK_RECOV | Time constant of the clock recovery (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
25:24 | DATARATE_OFFSET_DR_LIMIT | DATARATE_OFFSET_DR_LIMIT_DEFAULT |  | 0x0*
23:16 | DATARATE_OFFSET_DATARATE_OFFSET | DATARATE_OFFSET_DATARATE_OFFSET_DEFAULT | Signed value and the full scale (0x7f) corresponds to a data-rate offset of 12.5% | 0x0*
15:8 | TAU_DATARATE_RECOV_TAU_DATARATE_RECOV | TAU_DATARATE_RECOV_TAU_DATARATE_RECOV_DEFAULT |  | 0x20*
7:0 | TAU_CLK_RECOV_TAU_CLK_RECOV | TAU_CLK_RECOV_TAU_CLK_RECOV_DEFAULT |  | 0x9*