### LSAD_MONITOR_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
23:16 | RW | ALARM_COUNT_VALUE | An Alarm Status bit is set and an interrupt generated when SUPPLY_COUNT_VALUE = ALARM_COUNT_VALUE
15:8 | RW | MONITOR_THRESHOLD | Low voltage detection threshold (7.8 mV steps)
2:0 | RW | MONITOR_SRC | Selects the source channel to be monitored

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
23:16 | ALARM_COUNT_VALUE | MONITOR_ALARM_NONE | No Alarm is triggered | 0x0*
|  | MONITOR_ALARM_COUNT1 | Alarm count value is 1 | 0x1
|  | MONITOR_ALARM_COUNT255 | Alarm count value is 255 | 0xFF
15:8 | MONITOR_THRESHOLD | MONITOR_THRESHOLD_LOW | Lowest voltage threshold: 7.8 mV | 0x0
|  | MONITOR_THRESHOLD_MID | Mid voltage threshold: 1.4 V | 0xB3*
|  | MONITOR_THRESHOLD_HIGH | Highest voltage threshold: ~2.0 V | 0xFF
2:0 | MONITOR_SRC | MONITOR_CH0 | Channel 0 is monitored | 0x0
|  | MONITOR_CH1 | Channel 1 is monitored | 0x1
|  | MONITOR_CH2 | Channel 2 is monitored | 0x2
|  | MONITOR_CH3 | Channel 3 is monitored | 0x3
|  | MONITOR_CH4 | Channel 4 is monitored | 0x4
|  | MONITOR_CH5 | Channel 5 is monitored | 0x5
|  | MONITOR_CH6 | Channel 6 is monitored | 0x6
|  | MONITOR_CH7 | Channel 7 is monitored | 0x7*