### LSAD_INPUT_SEL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
6:4 | RW | POS_INPUT_SEL | Positive input selection
2:0 | RW | NEG_INPUT_SEL | Negative input selection

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
6:4 | POS_INPUT_SEL | LSAD_POS_INPUT_SEL0 | Select pre-selection input 0 as positive input | 0x0
|  | LSAD_POS_INPUT_SEL1 | Select pre-selection input 1 as positive input | 0x1
|  | LSAD_POS_INPUT_SEL2 | Select pre-selection input 2 as positive input | 0x2
|  | LSAD_POS_INPUT_SEL3 | Select pre-selection input 3 as positive input | 0x3
|  | LSAD_POS_INPUT_AOUT | Select AOUT as positive input | 0x4
|  | LSAD_POS_INPUT_TEMP | Select temperature sensor as positive input | 0x5
|  | LSAD_POS_INPUT_VBAT_DIV2 | Select VBAT/2 as positive input | 0x6*
|  | LSAD_POS_INPUT_GND | Select LSAD internal ground as positive input | 0x7
2:0 | NEG_INPUT_SEL | LSAD_NEG_INPUT_SEL0 | Select pre-selection input 0 as negative input | 0x0
|  | LSAD_NEG_INPUT_SEL1 | Select pre-selection input 1 as negative input | 0x1
|  | LSAD_NEG_INPUT_SEL2 | Select pre-selection input 2 as negative input | 0x2
|  | LSAD_NEG_INPUT_SEL3 | Select pre-selection input 3 as negative input | 0x3
|  | LSAD_NEG_INPUT_AOUT | Select AOUT as negative input | 0x4
|  | LSAD_NEG_INPUT_TEMP | Select temperature as negative input | 0x5
|  | LSAD_NEG_INPUT_VBAT_DIV2 | Select VBAT/2 as negative input | 0x6
|  | LSAD_NEG_INPUT_GND | Select LSAD internal ground as negative input | 0x7*