### TIMER_CFG0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
26:24 | RW | PRESCALE | Prescale value of the timer
23:0 | RW | TIMEOUT_VALUE | Number of Timer clock cycles to time-out

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
26:24 | PRESCALE | TIMER_PRESCALE_1 | Divide the input clock frequency by 1 | 0x0*
|  | TIMER_PRESCALE_2 | Divide the input clock frequency by 2 | 0x1
|  | TIMER_PRESCALE_4 | Divide the input clock frequency by 4 | 0x2
|  | TIMER_PRESCALE_8 | Divide the input clock frequency by 8 | 0x3
|  | TIMER_PRESCALE_16 | Divide the input clock frequency by 16 | 0x4
|  | TIMER_PRESCALE_32 | Divide the input clock frequency by 32 | 0x5
|  | TIMER_PRESCALE_64 | Divide the input clock frequency by 64 | 0x6
|  | TIMER_PRESCALE_128 | Divide the input clock frequency by 128 | 0x7