### BB_RADIOCNTL2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:30 | RW | LRSYNCCOMPMODE | Long-range synchronization compensation operating mode
29 | RW | RXCITERMBYPASS | Long-range CI bit[1] and TERM1 bypass mode (allow to receive only CI bit 0 and then wait for Rx payload directly)
28:24 | RW | LRVTBFLUSH | Indicate long range Viterbi flush instant (this value corresponds to the Viterbi trace back depth used in the selected design, hence corresponding to the number of remaining samples flush out just before the end of the packet)
23:22 | RW | PHYMSK | Indicate selected radio PHY support capabilities (in addition to 1Mbps that is mandatory)
21:20 | RW | LRSYNCERR | Number of errors allowed during long range Rx stream detection (when performed internally)
18:16 | RW | SYNCERR | Indicate the maximum number of errors allowed to recognize the synchronization word
13:0 | RW | FREQTABLE_PTR | Frequency table pointer

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:30 | LRSYNCCOMPMODE | LRSYNCCOMPMODE_3 | Bit 0 controls 125kbps LR packet part using synchro tracking and Bit 1 controls 500kbps LR packet part using synchro tracking | 0x3*
29 | RXCITERMBYPASS | RXCITERMBYPASS_0 |  | 0x0*
|  | RXCITERMBYPASS_1 |  | 0x1
28:24 | LRVTBFLUSH | LRVTBFLUSH_8 |  | 0x8*
23:22 | PHYMSK | PHYMSK_0 | Bit 0 indicates 2Mbps support when set. Bit 1 indicates Coded HPY support when set | 0x0*
21:20 | LRSYNCERR | LRSYNCERR_0 |  | 0x0*
18:16 | SYNCERR | SYNCERR_0 | Has to be set to 0x0 for normal operations | 0x0*
13:0 | FREQTABLE_PTR | FREQTABLE_PTR_64 |  | 0x40*