### RF_REG36

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
30:28 | RW | IQ_SPARES_EN_BIAS_SPARE | Enable for IQ spares
27:24 | RW | IQ_SPARES_IQ_SPARE_2 | Spare bias 2
23:20 | RW | IQ_SPARES_IQ_SPARE_1 | Spare bias 1
19:16 | RW | IQ_SPARES_IQ_SPARE_0 | Spare bias 0
8 | RW | MISC_ISO_VDDA | Isolate VDDA signals
5 | RW | BLR_DEMAPPER_BLR_SEND_DECODED_RI | Fully decode the rate indicator
4 | RW | BLR_DEMAPPER_BLR_USE_EXT_VIT_GFSK | 500kbps BLR uses the Viterbi GFSK decision
3:2 | RW | BLR_DEMAPPER_BLR_500_DPHASE | Set the distance between samples for the phase to frequency conversion in S2 mode
1 | RW | BLR_DEMAPPER_BLR_500_LOW_GAIN | Set the low gain in S2 mode
0 | RW | BLR_DEMAPPER_BLR_125_LOW_GAIN | Set the low gain in S8 mode

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
30:28 | IQ_SPARES_EN_BIAS_SPARE | IQ_SPARES_EN_BIAS_SPARE_DEFAULT |  | 0x0*
27:24 | IQ_SPARES_IQ_SPARE_2 | IQ_SPARES_IQ_SPARE_2_DEFAULT |  | 0x0*
23:20 | IQ_SPARES_IQ_SPARE_1 | IQ_SPARES_IQ_SPARE_1_DEFAULT |  | 0x0*
19:16 | IQ_SPARES_IQ_SPARE_0 | IQ_SPARES_IQ_SPARE_0_DEFAULT |  | 0x0*
8 | MISC_ISO_VDDA | MISC_ISO_VDDA_NOT_ISOLATE | Do not isolate VDDA signals | 0x0*
|  | MISC_ISO_VDDA_ISOLATE | Isolate VDDA signals | 0x1
5 | BLR_DEMAPPER_BLR_SEND_DECODED_RI | BLR_DEMAPPER_BLR_SEND_DECODED_RI_DISABLE | Rate indicator is not fully decoded and decision made is sent instead | 0x0*
|  | BLR_DEMAPPER_BLR_SEND_DECODED_RI_ENABLE | Rate indicator is fully decoded | 0x1
4 | BLR_DEMAPPER_BLR_USE_EXT_VIT_GFSK | BLR_DEMAPPER_BLR_USE_EXT_VIT_GFSK_DISABLE | Do not use the Viterbi GFSK decision | 0x0
|  | BLR_DEMAPPER_BLR_USE_EXT_VIT_GFSK_ENABLE | Use the Viterbi GFSK decision | 0x1*
3:2 | BLR_DEMAPPER_BLR_500_DPHASE | BLR_DEMAPPER_BLR_500_DPHASE_2 | 2 samples | 0x0
|  | BLR_DEMAPPER_BLR_500_DPHASE_4 | 4 samples | 0x1
|  | BLR_DEMAPPER_BLR_500_DPHASE_6 | 6 samples | 0x2
|  | BLR_DEMAPPER_BLR_500_DPHASE_8 | 8 samples | 0x3*
1 | BLR_DEMAPPER_BLR_500_LOW_GAIN | BLR_DEMAPPER_BLR_500_LOW_GAIN_DISABLE | Do not set low gain in S2 mode | 0x0*
|  | BLR_DEMAPPER_BLR_500_LOW_GAIN_ENABLE | Set low gain in S2 mode | 0x1
0 | BLR_DEMAPPER_BLR_125_LOW_GAIN | BLR_DEMAPPER_BLR_125_LOW_GAIN_DISABLE | Do not set low gain in S8 mode | 0x0*
|  | BLR_DEMAPPER_BLR_125_LOW_GAIN_ENABLE | Set low gain in S8 mode | 0x1